(footprint "FPC_Connector_1.0K-DX-18PWB"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "HDGC FPC Connector 1.0K-DX-18PWB")
	(tags "fpc, connector, flat cable")
	(property "Reference" "REF**"
		(at 9.1 -0.7 0)
		(layer "F.SilkS")
		(uuid "e7bf642b-2c82-4784-b19f-0da80a266795")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
			(justify left)
		)
	)
	(property "Value" "1.0K-ES-18PWB"
		(at 0 3.4 0)
		(layer "F.Fab")
		(uuid "c93d9188-b485-4f38-bd8d-e361be43063a")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "2acfbb90-3091-4c9e-b77e-e49d6fe4e5d9")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "552d8c0d-98f0-438c-9212-3cdf3876ed88")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -11.95 0)
		(end -11.95 0.5)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "c37b34f7-74be-4ced-8044-2fec3fab1d2c")
	)
	(fp_line
		(start -11.95 4.5)
		(end 11.95 4.5)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "c5daafde-52b4-4e6c-92d9-60cccb8521e5")
	)
	(fp_line
		(start -11.95 5.3)
		(end -11.95 3.3)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "271a8fdc-11a3-4ebb-bc2a-e6b453c28035")
	)
	(fp_line
		(start -11.95 5.3)
		(end 11.95 5.3)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "92da0955-3ae5-4704-b116-ba0c3c7d8f6a")
	)
	(fp_line
		(start -9 0)
		(end -11.95 0)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "c6f59a22-1b1f-434e-866c-5f508a33b693")
	)
	(fp_line
		(start 11.95 0)
		(end 9 0)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "f15f25f9-dc41-4cee-a546-1e7d0d4e94e7")
	)
	(fp_line
		(start 11.95 0)
		(end 11.95 0.5)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "6a6a5da4-d4ff-4388-b123-874566e87507")
	)
	(fp_line
		(start 11.95 5.3)
		(end 11.95 3.3)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "c75449c1-63f0-465b-9945-7a0c642c2e38")
	)
	(fp_poly
		(pts
			(xy -8.5 -1.8) (xy -8.7 -2.1) (xy -8.3 -2.1)
		)
		(stroke
			(width 0.12)
			(type solid)
		)
		(fill yes)
		(layer "F.SilkS")
		(uuid "44a0b012-1f14-4b1d-8cd9-bf2ead97bf27")
	)
	(fp_line
		(start -11.9 0)
		(end -9 0)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "44fa0da9-a920-4908-9b9b-336254e8b935")
	)
	(fp_line
		(start -11.9 5.2)
		(end -11.9 0)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "b366d63a-8106-4ebf-98f7-191c2a071b18")
	)
	(fp_line
		(start -9 -1.2)
		(end 9 -1.2)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "35aa8369-a77c-4e15-b27c-75675555f5c1")
	)
	(fp_line
		(start -9 0)
		(end -9 -1.2)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "d2641ec0-0219-4635-9814-e1b3eadb131b")
	)
	(fp_line
		(start 9 -1.2)
		(end 9 0)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "d8f3f8e7-f87a-4178-8a52-a458190460d8")
	)
	(fp_line
		(start 9 0)
		(end 11.9 0)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "327e577a-ba1c-4489-a540-b042efe173bf")
	)
	(fp_line
		(start 11.9 0)
		(end 11.9 5.2)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "ab56514f-192a-41b2-854b-905d095993ab")
	)
	(fp_line
		(start 11.9 5.2)
		(end -11.9 5.2)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "457e9ff2-93ce-428c-a61d-23eae0f1b5e4")
	)
	(fp_line
		(start -11.8 4.5)
		(end 11.8 4.5)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "8374212b-e32e-4a0c-9787-8d4b3fc0fab1")
	)
	(fp_line
		(start -8.5 0.4)
		(end -8.5 0.1)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "7f55ac70-2ad2-4748-9860-750517f94581")
	)
	(fp_line
		(start -7.5 0.4)
		(end -7.5 0.1)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "77c85094-2091-494f-9b61-4750fc81931d")
	)
	(fp_line
		(start -6.5 0.4)
		(end -6.5 0.1)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "419172e2-25af-4d38-9d92-a4136b631bfd")
	)
	(fp_line
		(start -5.5 0.4)
		(end -5.5 0.1)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "e9d1beee-c9cb-4120-96a6-1ebd6b5cbe08")
	)
	(fp_line
		(start -4.5 0.4)
		(end -4.5 0.1)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "08d30677-54d9-4ecb-b2ba-76ef4c5ec70a")
	)
	(fp_line
		(start -3.5 0.4)
		(end -3.5 0.1)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "86c254c6-5e41-411d-9c27-08c4a3383cac")
	)
	(fp_line
		(start -2.5 0.4)
		(end -2.5 0.1)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "3a484595-7f4f-4f03-b2f7-839c2ad54299")
	)
	(fp_line
		(start -1.5 0.4)
		(end -1.5 0.1)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "613c00a6-7d20-43a6-8060-35585d0c30c6")
	)
	(fp_line
		(start -0.5 0.4)
		(end -0.5 0.1)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "d6c88c8c-fa63-4ae3-a97c-ca349ffe7927")
	)
	(fp_line
		(start 0.5 0.4)
		(end 0.5 0.1)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "40a20ece-f173-4635-aa1b-4e2a9609b65a")
	)
	(fp_line
		(start 1.5 0.4)
		(end 1.5 0.1)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "04ea5475-46c5-4f23-b45e-7d2fe0a552d8")
	)
	(fp_line
		(start 2.5 0.4)
		(end 2.5 0.1)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "5e2564e3-631f-482c-b649-bf83a49d9a85")
	)
	(fp_line
		(start 3.5 0.4)
		(end 3.5 0.1)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "cd37e256-36f0-4ce4-ae7c-8fef69c0c161")
	)
	(fp_line
		(start 4.5 0.4)
		(end 4.5 0.1)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "de6c909e-420b-44bd-930c-1e323cad1801")
	)
	(fp_line
		(start 5.5 0.4)
		(end 5.5 0.1)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "78f1399e-385c-446b-b696-3a137f5c5b1b")
	)
	(fp_line
		(start 6.5 0.4)
		(end 6.5 0.1)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "82e3a8ea-f0b7-415c-8165-437e82e3ee7d")
	)
	(fp_line
		(start 7.5 0.4)
		(end 7.5 0.1)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "c492597f-52b5-423c-be87-5dc71db18cd6")
	)
	(fp_line
		(start 8.5 0.4)
		(end 8.5 0.1)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "0ebad8ac-94a5-4dc7-88d2-b81503ad21a4")
	)
	(fp_rect
		(start -11.8 5.2)
		(end 11.8 0.4)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill no)
		(layer "F.Fab")
		(uuid "cda4bc98-c8e2-43b7-b189-34581373d526")
	)
	(fp_text user "${REFERENCE}"
		(at 0 1.5 0)
		(layer "F.Fab")
		(uuid "940584f8-2632-4448-8ecc-84c1b7771847")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd rect
		(at -8.5 -0.7)
		(size 0.4 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "648b4f92-02f6-4388-8b44-e0bd13211b4b")
	)
	(pad "2" smd rect
		(at -7.5 -0.7)
		(size 0.4 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "c587fdb8-a9c6-413a-af84-e029beeac9fc")
	)
	(pad "3" smd rect
		(at -6.5 -0.7)
		(size 0.4 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "baf463e1-a7ec-46af-a928-638602ab9eb3")
	)
	(pad "4" smd rect
		(at -5.5 -0.7)
		(size 0.4 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "2fa6261c-0a55-418e-8748-b904ee7c2ee3")
	)
	(pad "5" smd rect
		(at -4.5 -0.7)
		(size 0.4 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "8c7d530d-de2f-42e7-a2c6-462a8f3f57b0")
	)
	(pad "6" smd rect
		(at -3.5 -0.7)
		(size 0.4 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "15dfc6eb-647b-4bab-be1f-15784ddced94")
	)
	(pad "7" smd rect
		(at -2.5 -0.7)
		(size 0.4 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "997254f3-9907-42f8-9ac5-cafb0ebb7bac")
	)
	(pad "8" smd rect
		(at -1.5 -0.7)
		(size 0.4 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "57ac7c76-668f-4e3b-83b6-63cf5246c036")
	)
	(pad "9" smd rect
		(at -0.5 -0.7)
		(size 0.4 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "3b474447-0733-49bf-a231-f0307be3145f")
	)
	(pad "10" smd rect
		(at 0.5 -0.7)
		(size 0.4 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "c7c82633-2911-41f1-bd1e-15e7de2fcfb1")
	)
	(pad "11" smd rect
		(at 1.5 -0.7)
		(size 0.4 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "7bc0e6d5-bb4d-4e27-8045-225d5e0f40e5")
	)
	(pad "12" smd rect
		(at 2.5 -0.7)
		(size 0.4 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "9ef7bd81-eeba-48ee-bdd7-42d5bb913444")
	)
	(pad "13" smd rect
		(at 3.5 -0.7)
		(size 0.4 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "9f7273ee-783e-469b-b5b9-03d9daf62b69")
	)
	(pad "14" smd rect
		(at 4.5 -0.7)
		(size 0.4 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "30ff1ce3-b50c-4ab8-9f69-2c41a62ab6b9")
	)
	(pad "15" smd rect
		(at 5.5 -0.7)
		(size 0.4 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "0e00ae85-6090-4ba0-8d69-f01497577aba")
	)
	(pad "16" smd rect
		(at 6.5 -0.7)
		(size 0.4 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "29537b48-52fa-4b71-b521-93119ded382c")
	)
	(pad "17" smd rect
		(at 7.5 -0.7)
		(size 0.4 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "511fdf43-6e3c-4091-b97b-b3f46f3158e5")
	)
	(pad "18" smd rect
		(at 8.5 -0.7)
		(size 0.4 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "7ab9cbff-ba6c-4466-83f0-12410f59fcb7")
	)
	(pad "MP" smd rect
		(at -11.25 1.9)
		(size 2.5 2.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "27811b89-de78-4e68-acbf-f61c1fd42478")
	)
	(pad "MP" smd rect
		(at 11.25 1.9)
		(size 2.5 2.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "181ff1a6-d7dc-4f65-b825-9d21ca11dbc7")
	)
	(embedded_fonts no)
	(model "${MY_ADDITIONS}/1.0K-DX-18PWB.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
