(footprint "Fuse_1812_4532Metric_Pad1.30x3.40mm_HandSolder"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Fuse SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://www.nikhef.nl/pub/departments/mt/projects/detectorR_D/dtddice/ERJ2G.pdf), generated with kicad-footprint-generator")
	(tags "fuse handsolder")
	(property "Reference" "REF**"
		(at 0 -2.65 0)
		(layer "F.SilkS")
		(uuid "08e3cc40-a961-4547-8b96-57a6010139e2")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "Fuse_1812_4532Metric_Pad1.30x3.40mm_HandSolder"
		(at 0 2.65 0)
		(layer "F.Fab")
		(uuid "8a71d230-fd0c-44f1-bc06-9a46f771681a")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "49ae98f2-e770-483c-bd65-6ba2ffaa64b2")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "2ef11570-a103-40e5-979d-e93d6408869f")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -1.386252 -1.71)
		(end 1.386252 -1.71)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "a0c9ffab-3db3-4171-ab74-2e36537ccba1")
	)
	(fp_line
		(start -1.386252 1.71)
		(end 1.386252 1.71)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "3d9794af-c6ad-42a9-a0e6-6f38ac8fc454")
	)
	(fp_line
		(start -3.12 -1.95)
		(end 3.12 -1.95)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "ca61d57d-1c61-45f2-8838-37f60da9368e")
	)
	(fp_line
		(start -3.12 1.95)
		(end -3.12 -1.95)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "297d40c6-5c20-42b3-88aa-914505b94f58")
	)
	(fp_line
		(start 3.12 -1.95)
		(end 3.12 1.95)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "c9a56dd4-514e-4a99-b86b-b64fe1eb5ac3")
	)
	(fp_line
		(start 3.12 1.95)
		(end -3.12 1.95)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "95e99304-6285-483a-9d75-019528fa0978")
	)
	(fp_line
		(start -2.25 -1.6)
		(end 2.25 -1.6)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "f725f17c-d744-4538-8bf8-ddb75e124a1e")
	)
	(fp_line
		(start -2.25 1.6)
		(end -2.25 -1.6)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "dab29ee6-2cb5-4d81-b74a-11beb3bd3a09")
	)
	(fp_line
		(start 2.25 -1.6)
		(end 2.25 1.6)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "90870a81-1bd0-4eb5-b3d8-0884615f8eca")
	)
	(fp_line
		(start 2.25 1.6)
		(end -2.25 1.6)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "e94e39de-c0da-4d30-b7eb-c8e1aeef5dfe")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
		(uuid "31a043f3-95df-4daf-aeab-2f9597299aa5")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd roundrect
		(at -2.225 0)
		(size 1.3 3.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.192308)
		(uuid "83a0d48f-ba11-4401-8828-0e7504307ded")
	)
	(pad "2" smd roundrect
		(at 2.225 0)
		(size 1.3 3.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.192308)
		(uuid "387f3196-a575-4511-83e7-110ec20cfe69")
	)
	(embedded_fonts no)
	(model "${MY_ADDITIONS}/fuse_smd1812.stp"
		(offset
			(xyz 0 0 1)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
