(footprint "LED_0805_2012Metric_diode_symbol"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
	(tags "LED")
	(property "Reference" "REF**"
		(at 0 -1.65 0)
		(layer "F.SilkS")
		(uuid "4bd5a48b-5afe-47ea-b18b-904e1316d68f")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "LED_0805_2012Metric_diode_symbol"
		(at 0 1.65 0)
		(layer "F.Fab")
		(uuid "a16933c9-8a05-4c8f-bab9-ec8b8683fe20")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "5143b7d6-d176-4fc5-9231-cd52a379dfe2")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "2c32907e-7ff8-4e95-9534-bfd602536e2e")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -1.685 -0.96)
		(end -1.685 0.96)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "d78523bd-232a-46b5-b2be-3f2c9158bc5a")
	)
	(fp_line
		(start -1.685 0.96)
		(end 1 0.96)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "ad1d269b-0db4-4f11-be92-2759439b12d4")
	)
	(fp_line
		(start -0.2 0.5)
		(end -0.2 -0.5)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "d4c5715f-43aa-4ea0-8538-b261fae2756c")
	)
	(fp_line
		(start 1 -0.96)
		(end -1.685 -0.96)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "edd959f3-dd30-4459-ad60-10da6d1d4836")
	)
	(fp_poly
		(pts
			(xy -0.2 0) (xy 0.2 -0.5) (xy 0.2 0.5)
		)
		(stroke
			(width 0.12)
			(type solid)
		)
		(fill yes)
		(layer "F.SilkS")
		(uuid "0956cfe6-5a37-4f4c-855d-77bf7f0ae846")
	)
	(fp_line
		(start -1.68 -0.95)
		(end 1.68 -0.95)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "dd780a25-078b-4bb6-b4cb-8ae3f62caebd")
	)
	(fp_line
		(start -1.68 0.95)
		(end -1.68 -0.95)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "a3292b67-1732-40be-a243-d1849cc97a10")
	)
	(fp_line
		(start 1.68 -0.95)
		(end 1.68 0.95)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "442130bb-46e7-4f6a-9e10-d17768ff7321")
	)
	(fp_line
		(start 1.68 0.95)
		(end -1.68 0.95)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "cc8fbbef-0e6f-4ac9-afa1-c58583bd3808")
	)
	(fp_line
		(start -1 -0.3)
		(end -1 0.6)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "b7269381-7e89-497a-9aa5-2d1209d057d4")
	)
	(fp_line
		(start -1 0.6)
		(end 1 0.6)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "11c2680d-63be-4bc9-ba58-40b16ad84484")
	)
	(fp_line
		(start -0.7 -0.6)
		(end -1 -0.3)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "53ec0470-abc5-43df-98a1-145848d5e109")
	)
	(fp_line
		(start -0.2 0.5)
		(end -0.2 -0.5)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.Fab")
		(uuid "349387cf-92d1-4b65-82ee-1fb53049d22d")
	)
	(fp_line
		(start 1 -0.6)
		(end -0.7 -0.6)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "4cb994ac-c874-4c05-898a-f479fc9e9878")
	)
	(fp_line
		(start 1 0.6)
		(end 1 -0.6)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "fc14d0ad-6a5a-4df3-8714-a66d4439ca82")
	)
	(fp_poly
		(pts
			(xy -0.2 0) (xy 0.2 -0.5) (xy 0.2 0.5)
		)
		(stroke
			(width 0.12)
			(type solid)
		)
		(fill yes)
		(layer "F.Fab")
		(uuid "c9d3686c-07d6-4d76-a48c-107449f32422")
	)
	(pad "1" smd roundrect
		(at -0.9375 0)
		(size 0.975 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "1b93e654-ec11-4f3e-b338-e1eb7d65f3ac")
	)
	(pad "2" smd roundrect
		(at 0.9375 0)
		(size 0.975 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "3ee78eb6-7330-4969-9c8c-cca05bb6f23e")
	)
	(embedded_fonts no)
	(model "${KICAD8_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
