(export (version D)
  (design
    (source G:\ownCloud\Projects\PCB-Heater\kicad\pcb-heater\pcb-heater.sch)
    (date "15.12.2021 18:36:26")
    (tool "Eeschema (5.1.9)-1")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source pcb-heater.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref U1)
      (value STM32G070RBTx)
      (footprint Package_QFP:LQFP-64_10x10mm_P0.5mm)
      (libsource (lib my_additions) (part STM32G070RBTx) (description "Mainstream Value line, Arm Cortex-M0+ MCU with 128 Kbytes of Flash memory, 36 Kbytes RAM, 64 MHz CPU, 4x USART, timers, ADC, comm. I/F, 2-3.6V, LQFP-64"))
      (sheetpath (names /) (tstamps /))
      (tstamp 61B8499F))
    (comp (ref J2)
      (value "Display module")
      (footprint Connector_PinSocket_2.54mm:PinSocket_1x16_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x16) (description "Generic connector, single row, 01x16, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 61B9055D))
    (comp (ref J7)
      (value Encoder)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x05) (description "Generic connector, single row, 01x05, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 61B88D47))
    (comp (ref PS1)
      (value HLK-PM03)
      (footprint Converter_ACDC:Converter_ACDC_HiLink_HLK-PMxx)
      (datasheet http://www.hlktech.net/product_detail.php?ProId=59)
      (libsource (lib Converter_ACDC) (part HLK-PM03) (description "Compact AC/DC board mount power module 3W 3V3"))
      (sheetpath (names /) (tstamps /))
      (tstamp 61B8F3F3))
    (comp (ref J4)
      (value 220V)
      (footprint TerminalBlock_Phoenix:TerminalBlock_Phoenix_MKDS-3-2-5.08_1x02_P5.08mm_Horizontal)
      (datasheet ~)
      (libsource (lib Connector) (part Screw_Terminal_01x02) (description "Generic screw terminal, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 61B90832))
    (comp (ref U3)
      (value LTV-814)
      (footprint my_additions:OPTO-SMD4)
      (datasheet https://optoelectronics.liteon.com/upload/download/DS-70-96-0013/LTV-8X4%20series%20201509.pdf)
      (libsource (lib Isolator) (part LTV-814) (description "AC/DC Optocoupler, Vce 35V, CTR 20%, DIP4"))
      (sheetpath (names /) (tstamps /))
      (tstamp 61B96906))
    (comp (ref R14)
      (value 10k)
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 61B9E9EC))
    (comp (ref R6)
      (value 47k)
      (footprint my_additions:R_0805_HandSolder_together_with_TH_8mm)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 61BA2758))
    (comp (ref R7)
      (value 47k)
      (footprint my_additions:R_0805_HandSolder_together_with_TH_8mm)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 61BA3C57))
    (comp (ref C3)
      (value 4u7)
      (footprint Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 61BA7E36))
    (comp (ref C4)
      (value 100n)
      (footprint Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 61BAA457))
    (comp (ref R17)
      (value 22)
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 61BF0F47))
    (comp (ref R18)
      (value 22)
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 61BF1CE7))
    (comp (ref R19)
      (value 22)
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 61BF22CC))
    (comp (ref C8)
      (value 100n)
      (footprint Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 61BF7126))
    (comp (ref Y1)
      (value 16MHz)
      (footprint my_additions:OSC-TH_L10.0-W4.5-P5.00)
      (datasheet ~)
      (libsource (lib Device) (part Crystal_Small) (description "Two pin crystal, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 61C1A44E))
    (comp (ref C1)
      (value 30p)
      (footprint Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 61C428FC))
    (comp (ref C2)
      (value 30p)
      (footprint Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 61C43B81))
    (comp (ref R5)
      (value 0)
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 61C45261))
    (comp (ref J8)
      (value i2c)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x04) (description "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 61C66109))
    (comp (ref U2)
      (value MAX6675)
      (footprint Package_SO:SO-8_3.9x4.9mm_P1.27mm)
      (datasheet https://datasheets.maximintegrated.com/en/ds/MAX6675.pdf)
      (libsource (lib my_additions) (part MAX6675) (description "Cold-Junction-Compensated K-Thermocoupleto-Digital Converter (0°C to +1024°C)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 61C8F235))
    (comp (ref C5)
      (value 100n)
      (footprint Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 61CCF73A))
    (comp (ref J6)
      (value TC)
      (footprint TerminalBlock_Phoenix:TerminalBlock_Phoenix_MKDS-3-2-5.08_1x02_P5.08mm_Horizontal)
      (datasheet ~)
      (libsource (lib Connector) (part Screw_Terminal_01x02) (description "Generic screw terminal, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 61CFFABD))
    (comp (ref Q1)
      (value LBC817)
      (footprint Package_TO_SOT_SMD:SOT-23_Handsoldering)
      (datasheet ~)
      (libsource (lib Device) (part Q_NPN_BEC) (description "NPN transistor, base/emitter/collector"))
      (sheetpath (names /) (tstamps /))
      (tstamp 61D399A8))
    (comp (ref R1)
      (value 220)
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 61D3C09B))
    (comp (ref BZ1)
      (value HNB09A03)
      (footprint my_additions:Buzzer_D9_H5.5)
      (datasheet ~)
      (libsource (lib Device) (part Buzzer) (description "Buzzer, polarized"))
      (sheetpath (names /) (tstamps /))
      (tstamp 61D3D7CB))
    (comp (ref R11)
      (value 120)
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 61D84483))
    (comp (ref R12)
      (value 120)
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 61D87224))
    (comp (ref R9)
      (value 10k)
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 61D9F793))
    (comp (ref R10)
      (value 10k)
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 61DA1286))
    (comp (ref J3)
      (value "SPI LCD")
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x03) (description "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 61DC7EDA))
    (comp (ref J5)
      (value Heater)
      (footprint TerminalBlock_Phoenix:TerminalBlock_Phoenix_MKDS-3-2-5.08_1x02_P5.08mm_Horizontal)
      (datasheet ~)
      (libsource (lib Connector) (part Screw_Terminal_01x02) (description "Generic screw terminal, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 61E4863D))
    (comp (ref U4)
      (value MOC3023M)
      (footprint my_additions:OPTO-SMD6)
      (datasheet https://www.onsemi.com/pub/Collateral/MOC3023M-D.PDF)
      (libsource (lib Relay_SolidState) (part MOC3023M) (description "Random Phase Opto-Triac, Vdrm 400V, Ift 5mA, DIP6"))
      (sheetpath (names /) (tstamps /))
      (tstamp 61E58893))
    (comp (ref Q3)
      (value BT138-600)
      (footprint Package_TO_SOT_THT:TO-220-3_Vertical)
      (datasheet https://assets.nexperia.com/documents/data-sheet/BT138_SER_D_E.pdf)
      (libsource (lib Triac_Thyristor) (part BT138-600) (description "12A RMS, 600V Off-State Voltage, Triac, TO-220"))
      (sheetpath (names /) (tstamps /))
      (tstamp 61E5AF19))
    (comp (ref R8)
      (value 270)
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 61E5D2C5))
    (comp (ref R15)
      (value 220)
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 61E906D6))
    (comp (ref R16)
      (value 470)
      (footprint my_additions:R_0805_HandSolder_together_with_TH_8mm)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 61E90889))
    (comp (ref D1)
      (value Green)
      (footprint LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part LED_Small) (description "Light emitting diode, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 61EE28FA))
    (comp (ref R2)
      (value 1k8)
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 61EF8313))
    (comp (ref J1)
      (value STOP)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x02) (description "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 61F2A440))
    (comp (ref Q2)
      (value LBC817)
      (footprint Package_TO_SOT_SMD:SOT-23_Handsoldering)
      (datasheet ~)
      (libsource (lib Device) (part Q_NPN_BEC) (description "NPN transistor, base/emitter/collector"))
      (sheetpath (names /) (tstamps /))
      (tstamp 61F6247F))
    (comp (ref R3)
      (value 220)
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 61F62485))
    (comp (ref C6)
      (value 470u)
      (footprint Capacitor_SMD:CP_Elec_6.3x7.7)
      (datasheet ~)
      (libsource (lib Device) (part CP_Small) (description "Polarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 61BA7675))
    (comp (ref C7)
      (value 100n)
      (footprint Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 61BA92D0))
    (comp (ref R4)
      (value 10k)
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 61C07348))
    (comp (ref R13)
      (value 220)
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 61E8F4A6))
    (comp (ref J9)
      (value SWD)
      (footprint Connector_PinHeader_1.27mm:PinHeader_2x07_P1.27mm_Vertical_SMD)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_02x07_Odd_Even) (description "Generic connector, double row, 02x07, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 61CD9E66))
    (comp (ref HS1)
      (value Heatsink_Pad)
      (footprint Heatsink:Heatsink_Fischer_SK104-STC-STIC_35x13mm_2xDrill2.5mm)
      (datasheet ~)
      (libsource (lib Mechanical) (part Heatsink_Pad) (description "Heatsink with electrical connection, 1 pin"))
      (sheetpath (names /) (tstamps /))
      (tstamp 61DF34FE))
    (comp (ref H1)
      (value MountingHole)
      (footprint MountingHole:MountingHole_3.2mm_M3_Pad_Via)
      (datasheet ~)
      (libsource (lib Mechanical) (part MountingHole) (description "Mounting Hole without connection"))
      (sheetpath (names /) (tstamps /))
      (tstamp 61E7A383))
    (comp (ref H2)
      (value MountingHole)
      (footprint MountingHole:MountingHole_3.2mm_M3_Pad_Via)
      (datasheet ~)
      (libsource (lib Mechanical) (part MountingHole) (description "Mounting Hole without connection"))
      (sheetpath (names /) (tstamps /))
      (tstamp 61E7C256))
    (comp (ref H3)
      (value MountingHole)
      (footprint MountingHole:MountingHole_3.2mm_M3_Pad_Via)
      (datasheet ~)
      (libsource (lib Mechanical) (part MountingHole) (description "Mounting Hole without connection"))
      (sheetpath (names /) (tstamps /))
      (tstamp 61E7C43D)))
  (libparts
    (libpart (lib Connector) (part Screw_Terminal_01x02)
      (description "Generic screw terminal, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp TerminalBlock*:*))
      (fields
        (field (name Reference) J)
        (field (name Value) Screw_Terminal_01x02))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))))
    (libpart (lib Connector_Generic) (part Conn_01x02)
      (description "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_1x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x02))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))))
    (libpart (lib Connector_Generic) (part Conn_01x03)
      (description "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_1x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x03))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))))
    (libpart (lib Connector_Generic) (part Conn_01x04)
      (description "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_1x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x04))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))))
    (libpart (lib Connector_Generic) (part Conn_01x05)
      (description "Generic connector, single row, 01x05, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_1x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x05))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))
        (pin (num 5) (name Pin_5) (type passive))))
    (libpart (lib Connector_Generic) (part Conn_01x16)
      (description "Generic connector, single row, 01x16, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_1x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x16))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))
        (pin (num 5) (name Pin_5) (type passive))
        (pin (num 6) (name Pin_6) (type passive))
        (pin (num 7) (name Pin_7) (type passive))
        (pin (num 8) (name Pin_8) (type passive))
        (pin (num 9) (name Pin_9) (type passive))
        (pin (num 10) (name Pin_10) (type passive))
        (pin (num 11) (name Pin_11) (type passive))
        (pin (num 12) (name Pin_12) (type passive))
        (pin (num 13) (name Pin_13) (type passive))
        (pin (num 14) (name Pin_14) (type passive))
        (pin (num 15) (name Pin_15) (type passive))
        (pin (num 16) (name Pin_16) (type passive))))
    (libpart (lib Connector_Generic) (part Conn_02x07_Odd_Even)
      (description "Generic connector, double row, 02x07, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_2x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_02x07_Odd_Even))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))
        (pin (num 5) (name Pin_5) (type passive))
        (pin (num 6) (name Pin_6) (type passive))
        (pin (num 7) (name Pin_7) (type passive))
        (pin (num 8) (name Pin_8) (type passive))
        (pin (num 9) (name Pin_9) (type passive))
        (pin (num 10) (name Pin_10) (type passive))
        (pin (num 11) (name Pin_11) (type passive))
        (pin (num 12) (name Pin_12) (type passive))
        (pin (num 13) (name Pin_13) (type passive))
        (pin (num 14) (name Pin_14) (type passive))))
    (libpart (lib Converter_ACDC) (part HLK-PM01)
      (aliases
        (alias HLK-PM03)
        (alias HLK-PM12)
        (alias HLK-PM24))
      (description "Compact AC/DC board mount power module 3W 5V")
      (docs http://www.hlktech.net/product_detail.php?ProId=54)
      (footprints
        (fp Converter*ACDC*HiLink*HLK?PM*))
      (fields
        (field (name Reference) PS)
        (field (name Value) HLK-PM01)
        (field (name Footprint) Converter_ACDC:Converter_ACDC_HiLink_HLK-PMxx))
      (pins
        (pin (num 1) (name AC/L) (type power_in))
        (pin (num 2) (name AC/N) (type power_in))
        (pin (num 3) (name -Vout) (type power_out))
        (pin (num 4) (name +Vout) (type power_out))))
    (libpart (lib Device) (part Buzzer)
      (description "Buzzer, polarized")
      (docs ~)
      (footprints
        (fp *Buzzer*))
      (fields
        (field (name Reference) BZ)
        (field (name Value) Buzzer))
      (pins
        (pin (num 1) (name -) (type passive))
        (pin (num 2) (name +) (type passive))))
    (libpart (lib Device) (part CP_Small)
      (description "Polarized capacitor, small symbol")
      (docs ~)
      (footprints
        (fp CP_*))
      (fields
        (field (name Reference) C)
        (field (name Value) CP_Small))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Device) (part C_Small)
      (description "Unpolarized capacitor, small symbol")
      (docs ~)
      (footprints
        (fp C_*))
      (fields
        (field (name Reference) C)
        (field (name Value) C_Small))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Device) (part Crystal_Small)
      (description "Two pin crystal, small symbol")
      (docs ~)
      (footprints
        (fp Crystal*))
      (fields
        (field (name Reference) Y)
        (field (name Value) Crystal_Small))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib Device) (part LED_Small)
      (description "Light emitting diode, small symbol")
      (docs ~)
      (footprints
        (fp LED*)
        (fp LED_SMD:*)
        (fp LED_THT:*))
      (fields
        (field (name Reference) D)
        (field (name Value) LED_Small))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib Device) (part Q_NPN_BEC)
      (description "NPN transistor, base/emitter/collector")
      (docs ~)
      (fields
        (field (name Reference) Q)
        (field (name Value) Q_NPN_BEC))
      (pins
        (pin (num 1) (name B) (type input))
        (pin (num 2) (name E) (type passive))
        (pin (num 3) (name C) (type passive))))
    (libpart (lib Device) (part R)
      (description Resistor)
      (docs ~)
      (footprints
        (fp R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Device) (part R_Small)
      (description "Resistor, small symbol")
      (docs ~)
      (footprints
        (fp R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R_Small))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Isolator) (part LTV-814)
      (description "AC/DC Optocoupler, Vce 35V, CTR 20%, DIP4")
      (docs https://optoelectronics.liteon.com/upload/download/DS-70-96-0013/LTV-8X4%20series%20201509.pdf)
      (footprints
        (fp DIP*W7.62mm*))
      (fields
        (field (name Reference) U)
        (field (name Value) LTV-814)
        (field (name Footprint) Package_DIP:DIP-4_W7.62mm))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))
        (pin (num 3) (name ~) (type passive))
        (pin (num 4) (name ~) (type passive))))
    (libpart (lib Mechanical) (part Heatsink_Pad)
      (description "Heatsink with electrical connection, 1 pin")
      (docs ~)
      (footprints
        (fp Heatsink_*))
      (fields
        (field (name Reference) HS)
        (field (name Value) Heatsink_Pad))
      (pins
        (pin (num 1) (name ~) (type passive))))
    (libpart (lib Mechanical) (part MountingHole)
      (description "Mounting Hole without connection")
      (docs ~)
      (footprints
        (fp MountingHole*))
      (fields
        (field (name Reference) H)
        (field (name Value) MountingHole)))
    (libpart (lib Relay_SolidState) (part MOC3010M)
      (aliases
        (alias MOC3011M)
        (alias MOC3012M)
        (alias MOC3020M)
        (alias MOC3021M)
        (alias MOC3022M)
        (alias MOC3023M)
        (alias MOC3051M)
        (alias MOC3052M))
      (description "Random Phase Opto-Triac, Vdrm 250V, Ift 15mA, DIP6")
      (docs https://www.onsemi.com/pub/Collateral/MOC3023M-D.PDF)
      (footprints
        (fp DIP*W7.62mm*)
        (fp SMDIP*W9.53mm*)
        (fp DIP*W10.16mm*))
      (fields
        (field (name Reference) U)
        (field (name Value) MOC3010M))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))
        (pin (num 3) (name NC) (type NotConnected))
        (pin (num 4) (name ~) (type passive))
        (pin (num 5) (name NC) (type NotConnected))
        (pin (num 6) (name ~) (type passive))))
    (libpart (lib Triac_Thyristor) (part TIC226)
      (aliases
        (alias TIC206)
        (alias BT138-600)
        (alias BT138-800)
        (alias TIC216)
        (alias BT136-500)
        (alias BT136-600)
        (alias BT136-800)
        (alias BT139-600)
        (alias BTA16-600B)
        (alias BTA16-600BW)
        (alias BTA16-600C)
        (alias BTA16-600CW)
        (alias BTA16-600SW)
        (alias BTA16-800B)
        (alias BTA16-800BW)
        (alias BTA16-800C)
        (alias BTA16-800CW)
        (alias BTA16-800SW)
        (alias BTB16-600B)
        (alias BTB16-600BW)
        (alias BTB16-600C)
        (alias BTB16-600CW)
        (alias BTB16-600SW)
        (alias BTB16-800B)
        (alias BTB16-800BW)
        (alias BTB16-800C)
        (alias BTB16-800CW)
        (alias BTB16-800SW))
      (description "8A RMS, 400-800V Off-State Voltage, Triac, TO-220")
      (docs http://pdf.datasheetcatalog.com/datasheet/PowerInnovations/mXuqxvy.pdf)
      (footprints
        (fp TO?220*))
      (fields
        (field (name Reference) Q)
        (field (name Value) TIC226)
        (field (name Footprint) Package_TO_SOT_THT:TO-220-3_Vertical))
      (pins
        (pin (num 1) (name A1) (type passive))
        (pin (num 2) (name A2) (type passive))
        (pin (num 3) (name G) (type input))))
    (libpart (lib my_additions) (part MAX6675)
      (description "Cold-Junction-Compensated K-Thermocoupleto-Digital Converter (0°C to +1024°C)")
      (docs https://datasheets.maximintegrated.com/en/ds/MAX6675.pdf)
      (fields
        (field (name Reference) U)
        (field (name Value) MAX6675)
        (field (name Footprint) Package_SO:SO-8_3.9x4.9mm_P1.27mm))
      (pins
        (pin (num 1) (name GND) (type power_in))
        (pin (num 2) (name T-) (type input))
        (pin (num 3) (name T+) (type input))
        (pin (num 4) (name VCC) (type power_in))
        (pin (num 5) (name SCK) (type BiDi))
        (pin (num 6) (name ~CS) (type BiDi))
        (pin (num 7) (name SO) (type BiDi))))
    (libpart (lib my_additions) (part STM32G070RBTx)
      (description "Mainstream Value line, Arm Cortex-M0+ MCU with 128 Kbytes of Flash memory, 36 Kbytes RAM, 64 MHz CPU, 4x USART, timers, ADC, comm. I/F, 2-3.6V, LQFP-64")
      (footprints
        (fp LQFP-64*10x10mm*P0.5mm*))
      (fields
        (field (name Reference) U)
        (field (name Value) STM32G070RBTx)
        (field (name Footprint) Package_QFP:LQFP-64_10x10mm_P0.5mm))
      (pins
        (pin (num 1) (name PC11) (type BiDi))
        (pin (num 2) (name PC12) (type BiDi))
        (pin (num 3) (name PC13) (type BiDi))
        (pin (num 4) (name PC14-OSC32_IN) (type BiDi))
        (pin (num 5) (name PC15-OSC32_OUT) (type BiDi))
        (pin (num 6) (name VBAT) (type power_in))
        (pin (num 7) (name VREF+) (type input))
        (pin (num 8) (name VDD) (type power_in))
        (pin (num 9) (name VSS) (type power_in))
        (pin (num 10) (name PF0-OSC_IN) (type BiDi))
        (pin (num 11) (name PF1-OSC_OUT) (type BiDi))
        (pin (num 12) (name NRST) (type input))
        (pin (num 13) (name PC0) (type BiDi))
        (pin (num 14) (name PC1) (type BiDi))
        (pin (num 15) (name PC2) (type BiDi))
        (pin (num 16) (name PC3) (type BiDi))
        (pin (num 17) (name PA0) (type BiDi))
        (pin (num 18) (name PA1) (type BiDi))
        (pin (num 19) (name PA2) (type BiDi))
        (pin (num 20) (name PA3) (type BiDi))
        (pin (num 21) (name PA4) (type BiDi))
        (pin (num 22) (name PA5) (type BiDi))
        (pin (num 23) (name PA6) (type BiDi))
        (pin (num 24) (name PA7) (type BiDi))
        (pin (num 25) (name PC4) (type BiDi))
        (pin (num 26) (name PC5) (type BiDi))
        (pin (num 27) (name PB0) (type BiDi))
        (pin (num 28) (name PB1) (type BiDi))
        (pin (num 29) (name PB2) (type BiDi))
        (pin (num 30) (name PB10) (type BiDi))
        (pin (num 31) (name PB11) (type BiDi))
        (pin (num 32) (name PB12) (type BiDi))
        (pin (num 33) (name PB13) (type BiDi))
        (pin (num 34) (name PB14) (type BiDi))
        (pin (num 35) (name PB15) (type BiDi))
        (pin (num 36) (name PA8) (type BiDi))
        (pin (num 37) (name PA9) (type BiDi))
        (pin (num 38) (name PC6) (type BiDi))
        (pin (num 39) (name PC7) (type BiDi))
        (pin (num 40) (name PD8) (type BiDi))
        (pin (num 41) (name PD9) (type BiDi))
        (pin (num 42) (name PA10) (type BiDi))
        (pin (num 43) (name PA11[PA9]) (type BiDi))
        (pin (num 44) (name PA12[PA10]) (type BiDi))
        (pin (num 45) (name PA13-SWDIO) (type BiDi))
        (pin (num 46) (name PA14-BOOT0-SWCLK) (type BiDi))
        (pin (num 47) (name PA15) (type BiDi))
        (pin (num 48) (name PC8) (type BiDi))
        (pin (num 49) (name PC9) (type BiDi))
        (pin (num 50) (name PD0) (type BiDi))
        (pin (num 51) (name PD1) (type BiDi))
        (pin (num 52) (name PD2) (type BiDi))
        (pin (num 53) (name PD3) (type BiDi))
        (pin (num 54) (name PD4) (type BiDi))
        (pin (num 55) (name PD5) (type BiDi))
        (pin (num 56) (name PD6) (type BiDi))
        (pin (num 57) (name PB3) (type BiDi))
        (pin (num 58) (name PB4) (type BiDi))
        (pin (num 59) (name PB5) (type BiDi))
        (pin (num 60) (name PB6) (type BiDi))
        (pin (num 61) (name PB7) (type BiDi))
        (pin (num 62) (name PB8) (type BiDi))
        (pin (num 63) (name PB9) (type BiDi))
        (pin (num 64) (name PC10) (type BiDi)))))
  (libraries
    (library (logical Connector)
      (uri D:\KiCad\share\kicad\library/Connector.lib))
    (library (logical Connector_Generic)
      (uri D:\KiCad\share\kicad\library/Connector_Generic.lib))
    (library (logical Converter_ACDC)
      (uri D:\KiCad\share\kicad\library/Converter_ACDC.lib))
    (library (logical Device)
      (uri D:\KiCad\share\kicad\library/Device.lib))
    (library (logical Isolator)
      (uri D:\KiCad\share\kicad\library/Isolator.lib))
    (library (logical Mechanical)
      (uri D:\KiCad\share\kicad\library/Mechanical.lib))
    (library (logical Relay_SolidState)
      (uri D:\KiCad\share\kicad\library/Relay_SolidState.lib))
    (library (logical Triac_Thyristor)
      (uri D:\KiCad\share\kicad\library/Triac_Thyristor.lib))
    (library (logical my_additions)
      (uri G:/ownCloud/Projects/kicad_libs/my_additions.lib)))
  (nets
    (net (code 1) (name +3V3)
      (node (ref J7) (pin 1))
      (node (ref R14) (pin 1))
      (node (ref U2) (pin 4))
      (node (ref PS1) (pin 4))
      (node (ref C5) (pin 1))
      (node (ref U1) (pin 7))
      (node (ref U1) (pin 8))
      (node (ref U1) (pin 6))
      (node (ref J2) (pin 2))
      (node (ref C4) (pin 1))
      (node (ref J8) (pin 1))
      (node (ref C3) (pin 1))
      (node (ref R4) (pin 1))
      (node (ref BZ1) (pin 1))
      (node (ref C7) (pin 1))
      (node (ref R10) (pin 1))
      (node (ref C6) (pin 1))
      (node (ref J9) (pin 3))
      (node (ref R9) (pin 1)))
    (net (code 2) (name LCD_SCK)
      (node (ref J3) (pin 1))
      (node (ref U1) (pin 57)))
    (net (code 3) (name LCD_MOSI)
      (node (ref J3) (pin 2))
      (node (ref U1) (pin 56)))
    (net (code 4) (name LCD_MISO)
      (node (ref J3) (pin 3))
      (node (ref U1) (pin 55)))
    (net (code 5) (name "Net-(J8-Pad2)")
      (node (ref J8) (pin 2))
      (node (ref R11) (pin 1)))
    (net (code 6) (name "Net-(J8-Pad3)")
      (node (ref J8) (pin 3))
      (node (ref R12) (pin 1)))
    (net (code 7) (name I2C1_SCL)
      (node (ref U1) (pin 62))
      (node (ref R11) (pin 2))
      (node (ref R9) (pin 2)))
    (net (code 8) (name I2C1_SDA)
      (node (ref U1) (pin 61))
      (node (ref R10) (pin 2))
      (node (ref R12) (pin 2)))
    (net (code 9) (name "Net-(R8-Pad1)")
      (node (ref U4) (pin 1))
      (node (ref R8) (pin 1)))
    (net (code 10) (name ZERO_CROSS)
      (node (ref R14) (pin 2))
      (node (ref U1) (pin 36))
      (node (ref U3) (pin 4)))
    (net (code 11) (name GATE_CONTROL)
      (node (ref R8) (pin 2))
      (node (ref U1) (pin 37)))
    (net (code 12) (name GND)
      (node (ref C1) (pin 2))
      (node (ref Q2) (pin 2))
      (node (ref J2) (pin 1))
      (node (ref U1) (pin 9))
      (node (ref J1) (pin 2))
      (node (ref D1) (pin 1))
      (node (ref C8) (pin 2))
      (node (ref J9) (pin 11))
      (node (ref J8) (pin 4))
      (node (ref U3) (pin 3))
      (node (ref U4) (pin 2))
      (node (ref C2) (pin 2))
      (node (ref C5) (pin 2))
      (node (ref PS1) (pin 3))
      (node (ref C3) (pin 2))
      (node (ref J7) (pin 5))
      (node (ref C4) (pin 2))
      (node (ref U2) (pin 1))
      (node (ref U2) (pin 2))
      (node (ref C7) (pin 2))
      (node (ref C6) (pin 2))
      (node (ref J6) (pin 2))
      (node (ref Q1) (pin 2))
      (node (ref J9) (pin 7))
      (node (ref J9) (pin 5)))
    (net (code 13) (name "Net-(R13-Pad1)")
      (node (ref R15) (pin 2))
      (node (ref R13) (pin 1)))
    (net (code 14) (name "Net-(Q3-Pad3)")
      (node (ref U4) (pin 4))
      (node (ref R16) (pin 2))
      (node (ref Q3) (pin 3)))
    (net (code 15) (name "Net-(R13-Pad2)")
      (node (ref R13) (pin 2))
      (node (ref U4) (pin 6)))
    (net (code 16) (name "Net-(Q1-Pad1)")
      (node (ref R1) (pin 1))
      (node (ref Q1) (pin 1)))
    (net (code 17) (name "Net-(U4-Pad3)")
      (node (ref U4) (pin 3)))
    (net (code 18) (name "Net-(U4-Pad5)")
      (node (ref U4) (pin 5)))
    (net (code 19) (name MAX_SCK)
      (node (ref U2) (pin 5))
      (node (ref U1) (pin 33)))
    (net (code 20) (name MAX_CS)
      (node (ref U2) (pin 6))
      (node (ref U1) (pin 35)))
    (net (code 21) (name MAX_MISO)
      (node (ref U1) (pin 34))
      (node (ref U2) (pin 7)))
    (net (code 22) (name BUZZER)
      (node (ref U1) (pin 63))
      (node (ref R1) (pin 2)))
    (net (code 23) (name "Net-(J6-Pad1)")
      (node (ref J6) (pin 1))
      (node (ref U2) (pin 3)))
    (net (code 24) (name "Net-(BZ1-Pad2)")
      (node (ref BZ1) (pin 2))
      (node (ref Q1) (pin 3)))
    (net (code 25) (name LCD_WR)
      (node (ref J2) (pin 5))
      (node (ref U1) (pin 28)))
    (net (code 26) (name LCD_CS)
      (node (ref U1) (pin 54))
      (node (ref J2) (pin 3)))
    (net (code 27) (name LCD_RS)
      (node (ref U1) (pin 27))
      (node (ref J2) (pin 4)))
    (net (code 28) (name LCD_RD)
      (node (ref J2) (pin 6))
      (node (ref U1) (pin 25)))
    (net (code 29) (name LCD_RST)
      (node (ref U1) (pin 26))
      (node (ref J2) (pin 7)))
    (net (code 30) (name LCD_LED)
      (node (ref R4) (pin 2))
      (node (ref J2) (pin 8))
      (node (ref Q2) (pin 3)))
    (net (code 31) (name "Net-(J9-Pad4)")
      (node (ref J9) (pin 4))
      (node (ref R17) (pin 2)))
    (net (code 32) (name "Net-(J9-Pad6)")
      (node (ref J9) (pin 6))
      (node (ref R18) (pin 2)))
    (net (code 33) (name "Net-(J9-Pad8)")
      (node (ref J9) (pin 8)))
    (net (code 34) (name "Net-(J9-Pad9)")
      (node (ref J9) (pin 9)))
    (net (code 35) (name "Net-(J9-Pad2)")
      (node (ref J9) (pin 2)))
    (net (code 36) (name "Net-(J9-Pad1)")
      (node (ref J9) (pin 1)))
    (net (code 37) (name "Net-(J9-Pad13)")
      (node (ref J9) (pin 13)))
    (net (code 38) (name "Net-(J9-Pad14)")
      (node (ref J9) (pin 14)))
    (net (code 39) (name "Net-(HS1-Pad1)")
      (node (ref HS1) (pin 1)))
    (net (code 40) (name "Net-(J9-Pad10)")
      (node (ref J9) (pin 10)))
    (net (code 41) (name "Net-(J9-Pad12)")
      (node (ref J9) (pin 12))
      (node (ref R19) (pin 2)))
    (net (code 42) (name LED_STATUS)
      (node (ref U1) (pin 15))
      (node (ref R2) (pin 2)))
    (net (code 43) (name "Net-(D1-Pad2)")
      (node (ref D1) (pin 2))
      (node (ref R2) (pin 1)))
    (net (code 44) (name STOP)
      (node (ref U1) (pin 16))
      (node (ref J1) (pin 1)))
    (net (code 45) (name LCD_LED_CTRL)
      (node (ref R3) (pin 2))
      (node (ref U1) (pin 14)))
    (net (code 46) (name "Net-(J5-Pad2)")
      (node (ref R15) (pin 1))
      (node (ref Q3) (pin 2))
      (node (ref J5) (pin 2)))
    (net (code 47) (name "Net-(U1-Pad49)")
      (node (ref U1) (pin 49)))
    (net (code 48) (name "Net-(U1-Pad40)")
      (node (ref U1) (pin 40)))
    (net (code 49) (name "Net-(U1-Pad41)")
      (node (ref U1) (pin 41)))
    (net (code 50) (name "Net-(U1-Pad5)")
      (node (ref U1) (pin 5)))
    (net (code 51) (name "Net-(U1-Pad4)")
      (node (ref U1) (pin 4)))
    (net (code 52) (name "Net-(U1-Pad3)")
      (node (ref U1) (pin 3)))
    (net (code 53) (name "Net-(U1-Pad2)")
      (node (ref U1) (pin 2)))
    (net (code 54) (name "Net-(U1-Pad1)")
      (node (ref U1) (pin 1)))
    (net (code 55) (name "Net-(U1-Pad64)")
      (node (ref U1) (pin 64)))
    (net (code 56) (name "Net-(U1-Pad53)")
      (node (ref U1) (pin 53)))
    (net (code 57) (name "Net-(U1-Pad48)")
      (node (ref U1) (pin 48)))
    (net (code 58) (name "Net-(U1-Pad39)")
      (node (ref U1) (pin 39)))
    (net (code 59) (name "Net-(U1-Pad38)")
      (node (ref U1) (pin 38)))
    (net (code 60) (name "Net-(U1-Pad13)")
      (node (ref U1) (pin 13)))
    (net (code 61) (name "Net-(U1-Pad47)")
      (node (ref U1) (pin 47)))
    (net (code 62) (name "Net-(U1-Pad44)")
      (node (ref U1) (pin 44)))
    (net (code 63) (name "Net-(U1-Pad43)")
      (node (ref U1) (pin 43)))
    (net (code 64) (name "Net-(U1-Pad42)")
      (node (ref U1) (pin 42)))
    (net (code 65) (name "Net-(Q2-Pad1)")
      (node (ref Q2) (pin 1))
      (node (ref R3) (pin 1)))
    (net (code 66) (name "Net-(U1-Pad30)")
      (node (ref U1) (pin 30)))
    (net (code 67) (name "Net-(U1-Pad31)")
      (node (ref U1) (pin 31)))
    (net (code 68) (name "Net-(U1-Pad32)")
      (node (ref U1) (pin 32)))
    (net (code 69) (name "Net-(U1-Pad29)")
      (node (ref U1) (pin 29)))
    (net (code 70) (name "Net-(U1-Pad50)")
      (node (ref U1) (pin 50)))
    (net (code 71) (name "Net-(U1-Pad51)")
      (node (ref U1) (pin 51)))
    (net (code 72) (name "Net-(U1-Pad52)")
      (node (ref U1) (pin 52)))
    (net (code 73) (name "Net-(J4-Pad1)")
      (node (ref R7) (pin 2))
      (node (ref R16) (pin 1))
      (node (ref Q3) (pin 1))
      (node (ref J4) (pin 1))
      (node (ref PS1) (pin 1)))
    (net (code 74) (name "Net-(R6-Pad1)")
      (node (ref U3) (pin 1))
      (node (ref R6) (pin 1)))
    (net (code 75) (name "Net-(J4-Pad2)")
      (node (ref R6) (pin 2))
      (node (ref PS1) (pin 2))
      (node (ref J4) (pin 2))
      (node (ref J5) (pin 1)))
    (net (code 76) (name "Net-(R7-Pad1)")
      (node (ref U3) (pin 2))
      (node (ref R7) (pin 1)))
    (net (code 77) (name "Net-(C1-Pad1)")
      (node (ref C1) (pin 1))
      (node (ref Y1) (pin 1))
      (node (ref U1) (pin 10)))
    (net (code 78) (name "Net-(J2-Pad9)")
      (node (ref J2) (pin 9))
      (node (ref U1) (pin 17)))
    (net (code 79) (name "Net-(J2-Pad10)")
      (node (ref U1) (pin 18))
      (node (ref J2) (pin 10)))
    (net (code 80) (name "Net-(J2-Pad11)")
      (node (ref U1) (pin 19))
      (node (ref J2) (pin 11)))
    (net (code 81) (name "Net-(J2-Pad12)")
      (node (ref J2) (pin 12))
      (node (ref U1) (pin 20)))
    (net (code 82) (name "Net-(J2-Pad13)")
      (node (ref U1) (pin 21))
      (node (ref J2) (pin 13)))
    (net (code 83) (name "Net-(J2-Pad14)")
      (node (ref J2) (pin 14))
      (node (ref U1) (pin 22)))
    (net (code 84) (name "Net-(J2-Pad15)")
      (node (ref U1) (pin 23))
      (node (ref J2) (pin 15)))
    (net (code 85) (name "Net-(J2-Pad16)")
      (node (ref J2) (pin 16))
      (node (ref U1) (pin 24)))
    (net (code 86) (name SWDIO)
      (node (ref R17) (pin 1))
      (node (ref U1) (pin 45)))
    (net (code 87) (name SWCLK)
      (node (ref R18) (pin 1))
      (node (ref U1) (pin 46)))
    (net (code 88) (name NRST)
      (node (ref U1) (pin 12))
      (node (ref R19) (pin 1))
      (node (ref C8) (pin 1)))
    (net (code 89) (name "Net-(C2-Pad1)")
      (node (ref Y1) (pin 2))
      (node (ref C2) (pin 1))
      (node (ref R5) (pin 2)))
    (net (code 90) (name "Net-(R5-Pad1)")
      (node (ref U1) (pin 11))
      (node (ref R5) (pin 1)))
    (net (code 91) (name ENC_DN)
      (node (ref J7) (pin 3))
      (node (ref U1) (pin 59)))
    (net (code 92) (name ENC_BTN)
      (node (ref J7) (pin 2))
      (node (ref U1) (pin 60)))
    (net (code 93) (name ENC_UP)
      (node (ref J7) (pin 4))
      (node (ref U1) (pin 58)))))