(footprint "SolderJumper-3_Open_roundpads_smaller_narrower"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(tags "jumper")
	(property "Reference" "REF**"
		(at 0 -1.4 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "d55c2b63-a50a-469c-916a-04d58eb5539b")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "SolderJumper-3_Open"
		(at 0.7 1.3 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "aba99e4e-0010-4ad9-b482-c0e6579a803a")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "5bdc9285-7c19-459d-be1f-6f2cf1a77264")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "12412177-1170-4bb4-9a52-2c709ef2818b")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr exclude_from_pos_files exclude_from_bom)
	(fp_poly
		(pts
			(xy -0.7 -0.4) (xy -0.4 -0.4) (xy -0.4 0.4) (xy -0.7 0.4)
		)
		(stroke
			(width 0)
			(type solid)
		)
		(fill yes)
		(layer "F.Mask")
		(uuid "621ea742-199a-40fb-b91d-0ae32f91de7a")
	)
	(fp_poly
		(pts
			(xy 0.4 -0.4) (xy 0.7 -0.4) (xy 0.7 0.4) (xy 0.4 0.4)
		)
		(stroke
			(width 0)
			(type solid)
		)
		(fill yes)
		(layer "F.Mask")
		(uuid "0b80aa9e-128f-433a-bd19-347d9f7cf138")
	)
	(fp_line
		(start -1.25 -0.5)
		(end 1.249999 -0.5)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "73567724-3325-4dfd-9545-e4e07e822258")
	)
	(fp_line
		(start 1.249999 0.5)
		(end -1.25 0.5)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "f8fa5bc2-57fe-4aad-aead-728a55d3691e")
	)
	(fp_arc
		(start -1.25 0.5)
		(mid -1.75 0)
		(end -1.25 -0.5)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "18e943c0-3e8d-4c9c-b390-f8e5b73a206a")
	)
	(fp_arc
		(start 1.249999 -0.5)
		(mid 1.749999 0)
		(end 1.249999 0.5)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "ecf2844e-297c-4ada-aceb-3c04e5fa4fe2")
	)
	(fp_text user "${REFERENCE}"
		(at 0.7 2.8 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "23d611c8-1165-47cb-83ac-b1d0f5525c2d")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd custom
		(at -0.975 0)
		(size 0.55 0.8)
		(layers "F.Cu" "F.Mask")
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_circle
				(center -0.275 0)
				(end 0.125 0)
				(width 0)
				(fill yes)
			)
		)
		(uuid "97cfc6f7-1f3d-4638-a90c-197b97745dac")
	)
	(pad "2" smd rect
		(at 0 0)
		(size 0.8 0.8)
		(layers "F.Cu" "F.Mask")
		(thermal_bridge_angle 45)
		(uuid "73ac92b6-6073-4007-913a-6396dedcc136")
	)
	(pad "3" smd custom
		(at 0.975 0 180)
		(size 0.55 0.8)
		(layers "F.Cu" "F.Mask")
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_circle
				(center -0.275 0)
				(end 0.125 0)
				(width 0)
				(fill yes)
			)
		)
		(uuid "55d37dae-cba5-4f67-b5f0-699a0f5c70ff")
	)
	(embedded_fonts no)
)
