(footprint "AD9833_module" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr through_hole)
  (fp_text reference "REF**" (at -1.27 -10.16 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify left))
    (tstamp 5ba78012-f3ac-4457-a37d-752b061d21fe)
  )
  (fp_text value "AD9833_module" (at 5.08 0 90 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp fde9c680-32bd-433f-9d42-4b8434be5e8b)
  )
  (fp_text user "VCC" (at 1.27 -7.62 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify left))
    (tstamp 0e2e132c-66cf-47c2-91b1-b96e08d87b6a)
  )
  (fp_text user "DGND" (at 1.27 -5.08 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify left))
    (tstamp 21b81f03-414c-413a-896e-375224996c1d)
  )
  (fp_text user "FSYNC" (at 1.27 2.54 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify left))
    (tstamp 2c87bcf0-8056-41f2-a2b9-6c36d2da0c1a)
  )
  (fp_text user "SDATA" (at 1.27 -2.54 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify left))
    (tstamp 6530ad8a-082f-4d1b-b85a-0ca305b520d9)
  )
  (fp_text user "OUT" (at 1.27 7.62 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify left))
    (tstamp d904366d-a12d-4e44-8c7a-97054d0c29da)
  )
  (fp_text user "SCLK" (at 1.27 0 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify left))
    (tstamp e9af602f-e3e5-40ea-824d-a433ac607632)
  )
  (fp_text user "AGND" (at 1.27 5.08 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify left))
    (tstamp ecc28562-bbc1-45d3-a04a-f23fbd04c2f0)
  )
  (fp_text user "${REFERENCE}" (at 2.667 0 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 75496e4a-4ea4-4c18-b939-2ecced90a6f2)
  )
  (fp_rect (start -1.5 -9.2) (end 10.9 9.2)
    (stroke (width 0.12) (type solid)) (fill none) (layer "F.SilkS") (tstamp accb2821-3a63-4f81-9129-53b914db993c))
  (fp_circle (center 8.35 -6.65) (end 9.9 -6.65)
    (stroke (width 0.12) (type solid)) (fill none) (layer "F.SilkS") (tstamp b035351e-d78e-4c6f-8555-cd41d4418901))
  (fp_circle (center 8.35 6.65) (end 9.9 6.65)
    (stroke (width 0.12) (type solid)) (fill none) (layer "F.SilkS") (tstamp e3256c2f-6f6c-4ce2-aa4a-5f8a08451ccd))
  (fp_rect (start -1.4986 -9.1948) (end 10.8966 9.1948)
    (stroke (width 0.12) (type solid)) (fill none) (layer "F.CrtYd") (tstamp cf45e511-b46c-40b7-ab15-e2d49afbef97))
  (fp_rect (start -1.5 -9.2) (end 10.9 9.2)
    (stroke (width 0.12) (type solid)) (fill none) (layer "F.Fab") (tstamp 827ea438-68be-4cf0-8f86-ea370d29e677))
  (fp_circle (center 8.35 -6.65) (end 9.9 -6.65)
    (stroke (width 0.12) (type solid)) (fill none) (layer "F.Fab") (tstamp a0cf454a-43f2-4c06-be4a-b69725b3688a))
  (fp_circle (center 8.35 6.65) (end 9.9 6.65)
    (stroke (width 0.12) (type solid)) (fill none) (layer "F.Fab") (tstamp bfb52c00-c74e-4bb5-a151-ad7551dced8c))
  (pad "1" thru_hole rect (at 0 -7.62) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (tstamp 8d327243-ec2d-4130-8031-8c23f68ee60c))
  (pad "2" thru_hole circle (at 0 -5.08) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (tstamp 29cb4d1b-6f76-45ea-87e4-3c05eb774a29))
  (pad "3" thru_hole circle (at 0 -2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (tstamp 3c0d401a-49d0-43df-bdd8-9ad86466b0fd))
  (pad "4" thru_hole circle (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (tstamp 7a952073-5663-43a7-b9fa-644f962a910a))
  (pad "5" thru_hole circle (at 0 2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (tstamp 8822ad42-fab7-44c0-9c1d-3d21d7276989))
  (pad "6" thru_hole circle (at 0 5.08) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (tstamp 09ab20fe-ebed-4b2c-bbae-30e4e38be796))
  (pad "7" thru_hole circle (at 0 7.62) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (tstamp 82dd5483-7fd9-44b8-a247-cf7467589735))
)
