(footprint "MP503_sensor"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "MP503 Air-Quality Gas Sensor")
	(tags "MP503 gas sensor")
	(property "Reference" "REF**"
		(at 0 -5.7 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "93633f31-f8d8-4b9e-adb9-2848beaa35bf")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "MP503"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "597a0c61-c0a0-4f3e-b491-08c29f0b0b6c")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" ""
		(at -2.3 -13.1 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "c8cca3c2-610a-446f-bca5-444d9e39020a")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at -2.3 -13.1 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "f475ca04-8405-4498-8267-9932a099b187")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at -2.3 -13.1 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "6858825a-5eca-43ed-83b2-ec7de39e949b")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole)
	(fp_line
		(start -0.5 5.6)
		(end -0.5 4.8)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "6e869131-4161-49eb-9266-177c70121454")
	)
	(fp_line
		(start -0.5 5.6)
		(end 0.5 5.6)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "54e1516a-e920-45b3-b253-e3210588fc57")
	)
	(fp_line
		(start 0.5 5.6)
		(end 0.5 4.8)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "5290625e-c68d-416c-8f9e-c05ed44ee048")
	)
	(fp_arc
		(start -0.5 4.8)
		(mid 0 -4.825971)
		(end 0.5 4.8)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "d9a91a72-1a78-4236-a273-8f6fce83101c")
	)
	(fp_circle
		(center 0 0)
		(end 3.2 0)
		(stroke
			(width 0.12)
			(type default)
		)
		(fill none)
		(layer "F.SilkS")
		(uuid "ab76d602-900f-4c04-8f41-55926bb957d7")
	)
	(fp_circle
		(center 0 0)
		(end 0 5.7)
		(stroke
			(width 0.12)
			(type default)
		)
		(fill none)
		(layer "F.CrtYd")
		(uuid "0b96cc2e-db44-4270-88ee-0a7d088ec566")
	)
	(fp_line
		(start -0.4 5.5)
		(end -0.4 4.7)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "11951562-6c89-4071-ac88-6f1c51d059a2")
	)
	(fp_line
		(start -0.4 5.5)
		(end 0.4 5.5)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "11402aa4-f59f-4ab7-b077-9880942fda0f")
	)
	(fp_line
		(start 0.4 5.5)
		(end 0.4 4.7)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "96e454ac-e902-4183-a156-ab2a5816a066")
	)
	(fp_circle
		(center 0 0)
		(end 3.2 0)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill none)
		(layer "F.Fab")
		(uuid "1cc512f6-434d-4df5-a222-56ab7676ed25")
	)
	(fp_circle
		(center 0 0)
		(end 4.7 0)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill none)
		(layer "F.Fab")
		(uuid "70b697b6-4b6b-460a-9f2c-39b8e1d7d3ee")
	)
	(fp_text user "${REFERENCE}"
		(at 0 -3.9 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "36175f66-9552-496a-8437-25265323cf4e")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" thru_hole circle
		(at -1.55 1.55)
		(size 1.6 1.6)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "60137053-b2e3-4e33-bc7d-b85140d78697")
	)
	(pad "2" thru_hole circle
		(at 1.55 1.55)
		(size 1.6 1.6)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "ead7b6ae-1b81-4111-99f0-683610c08be9")
	)
	(pad "3" thru_hole circle
		(at -1.55 -1.55)
		(size 1.6 1.6)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "ef5ca874-44fe-40de-8df0-063788766b43")
	)
	(pad "4" thru_hole circle
		(at 1.55 -1.55)
		(size 1.6 1.6)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "a548c30b-747a-4375-849c-145919715788")
	)
	(model "${my_additions}/MP503_sensor.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
