(footprint "KF7.62-03P"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "screw trminal block KF7.62")
	(tags "screw trminal block KF7.62 7.62")
	(property "Reference" "REF**"
		(at -11.79 -2.9 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "3e03811d-c15e-4cc8-bae4-a28c29cd0a30")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
			(justify left)
		)
	)
	(property "Value" "KF7.62-03P"
		(at 0 8.8 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "62caf2a9-8d32-4f37-b4e1-104b31f26b7d")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" ""
		(at 3.71 10.9 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "b527a6dd-870f-432b-86d3-7eacf1931422")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 3.71 10.9 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "a80a8bf0-5d27-4155-bd3d-9936e9ce8b20")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 3.71 10.9 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "ca05ac20-653e-4e40-8964-1fbcf7545862")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole)
	(fp_line
		(start -3.8 -2.1)
		(end -3.8 10.1)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "8229f86c-4f9d-4448-929a-8ac5e477b6db")
	)
	(fp_line
		(start 3.8 -2.1)
		(end 3.8 10.1)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "571261f2-9f95-402c-a01d-0bad45bfe5a8")
	)
	(fp_rect
		(start -11.53 -2.1)
		(end 11.53 10.1)
		(stroke
			(width 0.12)
			(type default)
		)
		(fill none)
		(layer "F.SilkS")
		(uuid "008b65bc-0dbf-4f1d-9700-3b235fd4255d")
	)
	(fp_rect
		(start -11.63 -2.2)
		(end 11.63 10.2)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill none)
		(layer "F.CrtYd")
		(uuid "f19b5b98-4540-4c58-b16f-87b595ec632b")
	)
	(fp_line
		(start -9.58 3.75)
		(end -7.87 3.75)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "630a9599-f57c-42a0-8432-65d0bcd1fa0c")
	)
	(fp_line
		(start -9.58 4.25)
		(end -7.87 4.25)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "6a37af4f-9127-42f4-ab5a-482cb771410a")
	)
	(fp_line
		(start -7.87 2.95)
		(end -7.37 2.95)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "3771392b-b92d-4487-80ec-ca18feb56638")
	)
	(fp_line
		(start -7.87 3.75)
		(end -7.87 2.95)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "e750811f-b9e5-432e-83a9-838a0b347ab5")
	)
	(fp_line
		(start -7.87 5.05)
		(end -7.87 4.25)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "3b22346e-af10-4a60-afe3-6bdd8152c06b")
	)
	(fp_line
		(start -7.87 5.05)
		(end -7.37 5.05)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "91a6aba0-f800-48c3-b610-3c800cdbe60f")
	)
	(fp_line
		(start -7.37 2.95)
		(end -7.37 3.75)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "16ded293-4384-4a2f-a173-5d9728bdfe56")
	)
	(fp_line
		(start -7.37 3.75)
		(end -5.66 3.75)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "fbec9ecd-6fa5-48dc-a705-64e1222deec9")
	)
	(fp_line
		(start -7.37 4.25)
		(end -7.37 5.05)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "e74f83c7-404c-48b8-a053-688e5f9026ea")
	)
	(fp_line
		(start -7.37 4.25)
		(end -5.66 4.25)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "25829aec-8742-4f15-bdd1-0eef7c4a45a8")
	)
	(fp_line
		(start -3.81 -2)
		(end -3.81 10)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "a0f99d5a-6244-4f99-b802-1332b1112f32")
	)
	(fp_line
		(start -1.96 3.75)
		(end -0.25 3.75)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "6241b0e7-d390-458b-a90f-5afb2f79e041")
	)
	(fp_line
		(start -1.96 4.25)
		(end -0.25 4.25)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "ab63b4a0-4377-40f1-9d13-f8b1eb6f3d41")
	)
	(fp_line
		(start -0.25 2.95)
		(end 0.25 2.95)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "4b744be2-b7d4-4bc5-bbba-fcdadbcd1f1f")
	)
	(fp_line
		(start -0.25 3.75)
		(end -0.25 2.95)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "04043a5e-a8e5-4519-8604-0d461b354307")
	)
	(fp_line
		(start -0.25 5.05)
		(end -0.25 4.25)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "89cff41e-d9b2-4075-9356-6f52ed7ac602")
	)
	(fp_line
		(start -0.25 5.05)
		(end 0.25 5.05)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "ebe05b7c-3843-422f-900a-6c25cd5fff9f")
	)
	(fp_line
		(start 0.25 2.95)
		(end 0.25 3.75)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "0dd3402d-92e5-49ed-9c93-1981f3ea82c2")
	)
	(fp_line
		(start 0.25 3.75)
		(end 1.96 3.75)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "595e69dd-b527-458a-984e-3040a6a4935a")
	)
	(fp_line
		(start 0.25 4.25)
		(end 0.25 5.05)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "4aa8ef6e-bace-4f6d-a30c-1dfb130dbab9")
	)
	(fp_line
		(start 0.25 4.25)
		(end 1.96 4.25)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "305e3d64-35a8-4e14-9c54-d896bbce3060")
	)
	(fp_line
		(start 3.81 -2)
		(end 3.81 10)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "94b60884-1a65-4cb4-9195-1f2fd73afa85")
	)
	(fp_line
		(start 5.66 3.75)
		(end 7.37 3.75)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "07f3347d-5017-4e33-bc27-c351e618e5a9")
	)
	(fp_line
		(start 5.66 4.25)
		(end 7.37 4.25)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "b1bf5abe-d63b-487b-b920-43cf0ae24f9a")
	)
	(fp_line
		(start 7.37 2.95)
		(end 7.87 2.95)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "96d5353b-acff-49b9-a1af-ab03699342c7")
	)
	(fp_line
		(start 7.37 3.75)
		(end 7.37 2.95)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "8ee56d3c-2d30-468d-8cec-3fc58a8361f5")
	)
	(fp_line
		(start 7.37 5.05)
		(end 7.37 4.25)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "ee25dcb0-0e71-4c69-b143-9b7f0ad4b429")
	)
	(fp_line
		(start 7.37 5.05)
		(end 7.87 5.05)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "7db4d644-8159-4707-beb7-d3702502eff4")
	)
	(fp_line
		(start 7.87 2.95)
		(end 7.87 3.75)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "66c282d9-005e-4f16-87ee-590bbe3578a9")
	)
	(fp_line
		(start 7.87 3.75)
		(end 9.58 3.75)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "eb4651e1-2715-42bb-b996-a0b7beb2a557")
	)
	(fp_line
		(start 7.87 4.25)
		(end 7.87 5.05)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "472f661c-5517-4ac8-af97-51a6733dc9cc")
	)
	(fp_line
		(start 7.87 4.25)
		(end 9.58 4.25)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "0017b8b7-1300-407b-b23e-5a0ea6ebe7f2")
	)
	(fp_rect
		(start -11.43 10)
		(end 11.43 -2)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill none)
		(layer "F.Fab")
		(uuid "f3699a53-8e44-4844-8d91-a98513618002")
	)
	(fp_circle
		(center -7.62 4)
		(end -5.62 4)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill none)
		(layer "F.Fab")
		(uuid "f9b4d7b8-e16e-401d-8433-bfab27deeef6")
	)
	(fp_circle
		(center 0 4)
		(end 2 4)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill none)
		(layer "F.Fab")
		(uuid "51819a89-e944-42c0-9836-b6b21964eb15")
	)
	(fp_circle
		(center 7.62 4)
		(end 9.62 4)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill none)
		(layer "F.Fab")
		(uuid "0f423b09-8ec9-4eaa-8753-28f33910250c")
	)
	(fp_text user "${REFERENCE}"
		(at 0 7 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "6f46b683-ef27-4f8d-9ecb-c4158eb00a78")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" thru_hole circle
		(at -7.62 0)
		(size 3.8 3.8)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "f8cc9d21-1cff-40cc-b7e9-298e0ca13d3e")
	)
	(pad "2" thru_hole circle
		(at 0 0)
		(size 3.8 3.8)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "a14bb26a-a72a-423e-af44-63edbaca7b98")
	)
	(pad "3" thru_hole circle
		(at 7.62 0)
		(size 3.8 3.8)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "1eca0434-d921-4953-a18c-3b144924fe84")
	)
	(model "${my_additions}/KF7.62-3P.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
