(footprint "LED_matrix_8x8-60.2x60.2mm"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "8x8 LED matrix 2088")
	(tags "LED matrix")
	(property "Reference" "REF**"
		(at -20.955 -53.975 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "3fdcfeff-9e5c-488e-b260-d4c4ec12dc9c")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
			(justify left)
		)
	)
	(property "Value" "LED_matrix_8x8-60.2x60.2mm"
		(at 8.89 -23.725 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "c8101c54-44b3-4b3f-9fe7-c4c5b8e7e13e")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" ""
		(at 8.89 -24.725 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "9c3eac20-9ceb-4612-ba78-97801ab62713")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 8.89 -24.725 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "24545ab3-8324-4738-8fb8-d1690ac709c8")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 8.89 -24.725 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "b222b8d8-e080-4d48-8868-f8f329f170f9")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole)
	(fp_rect
		(start -21.21 -52.96)
		(end 38.99 7.24)
		(stroke
			(width 0.12)
			(type default)
		)
		(fill none)
		(layer "F.SilkS")
		(uuid "53a50006-7eaa-4948-8182-118b2b43a79b")
	)
	(fp_line
		(start -21.21 -52.96)
		(end -14.21 -52.96)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "8e3855a2-251b-439c-82e2-aa25db9ff6dc")
	)
	(fp_line
		(start -21.21 -45.96)
		(end -21.21 -52.96)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "de3c41a6-d362-4701-92d5-261f67256d1a")
	)
	(fp_line
		(start -21.21 0.24)
		(end -19.61 0.24)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "eea66565-936c-429b-a36f-3058bd4e3c51")
	)
	(fp_line
		(start -21.21 7.24)
		(end -21.21 0.24)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "93d879e1-bb47-445d-8c50-24c8aff2c833")
	)
	(fp_line
		(start -19.61 -51.36)
		(end -19.61 -45.96)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "502cef24-16f6-47ff-9525-73b8bb71fefb")
	)
	(fp_line
		(start -19.61 -45.96)
		(end -21.21 -45.96)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "5ed76512-a2a8-4acc-8c40-62d193abfcc1")
	)
	(fp_line
		(start -19.61 0.24)
		(end -19.61 5.64)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "19391bfc-eff3-45ea-95a6-74733dd623c4")
	)
	(fp_line
		(start -19.61 5.64)
		(end -14.21 5.64)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "c99cf142-8948-476f-b1ff-31b128d005a1")
	)
	(fp_line
		(start -14.21 -52.96)
		(end -14.21 -51.36)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "d7a21ee6-e5a9-4eac-8c34-3fd0ffe8bce9")
	)
	(fp_line
		(start -14.21 -51.36)
		(end -19.61 -51.36)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "1c0085b6-6ebd-4924-b6c8-70e0f97fa0db")
	)
	(fp_line
		(start -14.21 5.64)
		(end -14.21 7.24)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "585cb39f-e078-49de-9970-fa4cb6c285c6")
	)
	(fp_line
		(start -14.21 7.24)
		(end -21.21 7.24)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "065b12c6-cec3-4147-aa39-018543cab298")
	)
	(fp_line
		(start 31.99 -52.96)
		(end 38.99 -52.96)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "7f9c31ea-fbcc-4bdd-9130-5da923143ce6")
	)
	(fp_line
		(start 31.99 -51.36)
		(end 31.99 -52.96)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "3fc3664b-2128-43d3-8257-bfb36ccccd7b")
	)
	(fp_line
		(start 31.99 5.64)
		(end 37.39 5.64)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "68aff84c-6386-48a2-8b1f-dc55db7e959b")
	)
	(fp_line
		(start 31.99 7.24)
		(end 31.99 5.64)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "c30c7fe0-14d0-4196-a27e-b2e67f9c098e")
	)
	(fp_line
		(start 37.39 -51.36)
		(end 31.99 -51.36)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "aa968b16-1850-4eb6-a55b-7929da979981")
	)
	(fp_line
		(start 37.39 -45.96)
		(end 37.39 -51.36)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "666db491-967e-4a40-9dde-5855052b8df4")
	)
	(fp_line
		(start 37.39 0.24)
		(end 38.99 0.24)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "4dec8d23-fe43-4acf-b862-a7a969ba3e98")
	)
	(fp_line
		(start 37.39 5.64)
		(end 37.39 0.24)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "a4b7c537-522c-473e-8837-a019a8e791fd")
	)
	(fp_line
		(start 38.99 -52.96)
		(end 38.99 -45.96)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "04fe2436-d93f-4ea8-90b8-44e7fc7f8bc9")
	)
	(fp_line
		(start 38.99 -45.96)
		(end 37.39 -45.96)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "6e2a7042-d659-434b-b8dd-6292b4ad4e24")
	)
	(fp_line
		(start 38.99 0.24)
		(end 38.99 7.24)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "2eb25359-c231-4892-a031-99d84384d36c")
	)
	(fp_line
		(start 38.99 7.24)
		(end 31.99 7.24)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "93fe2ee1-998c-430c-a062-600060d8d05a")
	)
	(fp_rect
		(start -21.21 -52.96)
		(end 38.99 7.24)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill none)
		(layer "F.Fab")
		(uuid "c3dca4d3-002e-46d2-94ed-5a9d03b85e0a")
	)
	(fp_text user "${REFERENCE}"
		(at 8.89 -22.225 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "794ac0b3-1b26-445c-99cb-c36f7a422e01")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" thru_hole roundrect
		(at 0 0)
		(size 1.6 1.6)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.09375)
		(uuid "1d08b258-f1b1-452e-9cd7-45cf5eb92dfa")
	)
	(pad "2" thru_hole circle
		(at 2.54 0)
		(size 1.6 1.6)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "1694b640-d124-4e52-aa51-94f535b0fe17")
	)
	(pad "3" thru_hole circle
		(at 5.08 0)
		(size 1.6 1.6)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "abf791ec-739f-4b46-aa00-f8fd9fbcede7")
	)
	(pad "4" thru_hole circle
		(at 7.62 0)
		(size 1.6 1.6)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "a17d260b-d72d-4ec4-bb82-a19a69b95962")
	)
	(pad "5" thru_hole circle
		(at 10.16 0)
		(size 1.6 1.6)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "565f08d8-72be-4b3a-aabf-a0298cfa57c5")
	)
	(pad "6" thru_hole circle
		(at 12.7 0)
		(size 1.6 1.6)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "2362ecd3-45d8-4aff-b838-bb33194315d1")
	)
	(pad "7" thru_hole circle
		(at 15.24 0)
		(size 1.6 1.6)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "7b0f1d42-d787-478b-be4b-ba4724e802a7")
	)
	(pad "8" thru_hole circle
		(at 17.78 0)
		(size 1.6 1.6)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "d5eb3380-a305-46c4-9869-991a3ebcaaa0")
	)
	(pad "9" thru_hole circle
		(at 17.78 -45.72)
		(size 1.6 1.6)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "6c0fc0fd-f816-49af-87d5-62cb0edc876c")
	)
	(pad "10" thru_hole circle
		(at 15.24 -45.72)
		(size 1.6 1.6)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "ae386437-b086-46cf-92b2-394eba2d9ef9")
	)
	(pad "11" thru_hole circle
		(at 12.7 -45.72)
		(size 1.6 1.6)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "85825d11-daa3-45f0-a348-bc70823ff1e8")
	)
	(pad "12" thru_hole circle
		(at 10.16 -45.72)
		(size 1.6 1.6)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "b2644d3d-e3ec-45cc-9577-c2d563902ac9")
	)
	(pad "13" thru_hole circle
		(at 7.62 -45.72)
		(size 1.6 1.6)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "7d8a1048-c644-4486-82fb-23b58450ceb7")
	)
	(pad "14" thru_hole circle
		(at 5.08 -45.72)
		(size 1.6 1.6)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "4c527642-824f-474e-919c-61c189c2241f")
	)
	(pad "15" thru_hole circle
		(at 2.54 -45.72)
		(size 1.6 1.6)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "88090f07-8e40-46a4-942e-72211a71f3ee")
	)
	(pad "16" thru_hole circle
		(at 0 -45.72)
		(size 1.6 1.6)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "77b5b22a-d467-4590-964b-c68af9c751b2")
	)
	(model "${my_additions}/LED_matrix_8x8-60.2x60.2mm.stp"
		(offset
			(xyz 17.78 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 -90)
		)
	)
)
