(module mouse-bite-1mm-slot (layer F.Cu) (tedit 551DB9EF)
  (fp_text reference mouse-bite-1mm-slot (at 0 -2) (layer F.SilkS) hide
    (effects (font (size 1 1) (thickness 0.2)))
  )
  (fp_text value VAL** (at 0 2.1) (layer F.SilkS) hide
    (effects (font (size 1 1) (thickness 0.2)))
  )
  (fp_circle (center 1.5 0) (end 1.56 0) (layer Dwgs.User) (width 0.05))
  (fp_circle (center -1.5 0) (end -1.44 0) (layer Dwgs.User) (width 0.05))
  (fp_arc (start 1.5 0) (end 1.5 0.5) (angle 180) (layer F.SilkS) (width 0.1))
  (fp_arc (start -1.5 0) (end -1.5 -0.5) (angle 180) (layer F.SilkS) (width 0.1))
  (fp_line (start -1.5 0) (end -1.5 0) (layer Eco1.User) (width 1))
  (fp_line (start 1.5 0) (end 1.5 0) (layer Eco1.User) (width 1))
  (pad "" np_thru_hole circle (at 0.35 -1) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at -1.15 0.75) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at 1.15 0.75) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at -1.15 -0.75) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at -0.35 -1) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at 1.15 -0.75) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at -0.35 1) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at 0.35 1) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
)
