(footprint "Transform_D_26.9_14.7_11.2_one_coil_v4_Vertical" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "Transformer on a toroidal core D26.9/14.7/11.2 one coil Horizontal")
  (tags "transformer, toroidal")
  (attr through_hole)
  (fp_text reference "REF**" (at -6.2 -14.8) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify left))
    (tstamp 24e67e86-dfbe-4e5c-bc34-e48aa0ad80ed)
  )
  (fp_text value "Transform_D_26.9_14.7_11.2_one_coil_v4_Vertical" (at 9.2 0 90 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp a66e89f7-244a-48df-a0ce-c24530f40c45)
  )
  (fp_text user "${REFERENCE}" (at 0 -0.1 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 3a022eb6-748d-44d9-9d78-1f97a1218823)
  )
  (fp_line (start -6 -14) (end -6 8.7)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp a1cb98df-92d8-419e-ae8e-f1c13b8c6c89))
  (fp_line (start -6 13.3) (end -6 14)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp e48f9141-08ce-47bb-b5ea-4aec39b3b38c))
  (fp_line (start -6 14) (end 6 14)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 35baee7c-0fd5-47a4-a139-186f2a215ff2))
  (fp_line (start 6 -14) (end -6 -14)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 6d6a1985-04c3-4615-858d-cbb22f0ff5b0))
  (fp_line (start 6 -0.5) (end 6 -14)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 7dcdf47e-dbca-4c16-a451-4b45fff4f532))
  (fp_line (start 6 14) (end 6 4.1)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp b65a9fbc-14e2-44b3-a39c-91099ddf54bc))
  (fp_rect (start -8 -16) (end 8 16)
    (stroke (width 0.12) (type default)) (fill none) (layer "F.CrtYd") (tstamp 14a13a5a-ce3b-4a97-b60f-bfee70bd89d2))
  (fp_rect (start -5.9 -13.9) (end 5.9 13.9)
    (stroke (width 0.1) (type default)) (fill none) (layer "F.Fab") (tstamp fb7b235d-8632-48e3-a667-04d1bcb49d04))
  (pad "1" thru_hole circle (at 6.5 1.8) (size 4 4) (drill 2) (layers "*.Cu" "*.Mask") (tstamp 9b089a06-6942-4750-9e58-c020a7366b9d))
  (pad "2" thru_hole circle (at -6.5 11) (size 4 4) (drill 2) (layers "*.Cu" "*.Mask") (tstamp b70d2c14-8515-4d01-84e7-2f05b819a57a))
  (model "${my_additions}/Tor_core_D_26.9_14.7_11.2.step"
    (offset (xyz 5.5 0 15.5))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 90 0))
  )
)
