(footprint "MQ131"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0.1 -9.4 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "6d61b79f-3ae4-4b20-b550-e3a588598a13")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "MQ131"
		(at 0 -0.8 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "fcd2d214-a620-47e8-b236-53ec18fb7adb")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" ""
		(at -25 -17.9 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "541c6bfd-ebdc-4d59-b13c-7781fa909c5b")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at -25 -17.9 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "d03b5015-a7e2-4ab7-afe2-c062909bac55")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at -25 -17.9 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "f9ab45ad-48be-4c39-933d-f1f7cca568b5")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole)
	(fp_circle
		(center 0 0)
		(end 8.1 0)
		(stroke
			(width 0.12)
			(type default)
		)
		(fill none)
		(layer "F.SilkS")
		(uuid "411eb878-ca03-4cb3-93af-ccfe3213b1d4")
	)
	(fp_circle
		(center 0 0)
		(end 8.2 0)
		(stroke
			(width 0.12)
			(type default)
		)
		(fill none)
		(layer "F.CrtYd")
		(uuid "a7e507e0-f608-46c0-ad37-d09d43e52cc6")
	)
	(fp_circle
		(center 0 0)
		(end 8 0)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill none)
		(layer "F.Fab")
		(uuid "3825838d-9942-4f7a-92db-e26859e6bea9")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0.7 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "418dd614-b372-4921-990e-f6bead97d60a")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" thru_hole circle
		(at -3.36 -3.35876)
		(size 2.4 2.4)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "ec1d0822-a122-490d-9689-67e72cf42476")
	)
	(pad "2" thru_hole circle
		(at -4.75 0)
		(size 2.4 2.4)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "91ab9974-e9ed-4911-ad37-32a5a61fd7c8")
	)
	(pad "3" thru_hole circle
		(at -3.35876 3.35876)
		(size 2.4 2.4)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "7be24664-e7b4-4e7a-ab9e-ec125730d366")
	)
	(pad "4" thru_hole circle
		(at 3.35876 3.35876)
		(size 2.4 2.4)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "7852a949-28ab-4bba-8fdb-e8c2d65fd006")
	)
	(pad "5" thru_hole circle
		(at 4.75 0)
		(size 2.4 2.4)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "6b7fd7d8-dffb-4d1b-8194-e5492e4a46b6")
	)
	(pad "6" thru_hole circle
		(at 3.35876 -3.35876)
		(size 2.4 2.4)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "9068d220-3958-46ab-be08-4433b3d4d069")
	)
	(model "${my_additions}/MQ131.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
