(footprint "WOM_package" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 0)
  (descr "Diode bridge")
  (attr through_hole)
  (fp_text reference "REF**" (at 0 -5.715 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp ddf05a4f-e943-4ccb-8663-211a5801342a)
  )
  (fp_text value "WOM_package" (at -0.2 5.715 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp c2ee1014-353b-41ea-9939-8696768d0893)
  )
  (fp_text user "~" (at -1.905 1.27 unlocked) (layer "F.SilkS")
    (effects (font (size 1.5 1.5) (thickness 0.15)))
    (tstamp 37324c33-ae76-4bb6-8c66-90485cb32bd9)
  )
  (fp_text user "-" (at 1.905 1.27 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 5eb19350-4d6b-46e7-b4fb-8f757292ce66)
  )
  (fp_text user "~" (at 1.905 -1.27 unlocked) (layer "F.SilkS")
    (effects (font (size 1.5 1.5) (thickness 0.15)))
    (tstamp a0a4cd85-cc57-4538-8489-24e1fa6aad48)
  )
  (fp_text user "+" (at -1.905 -1.27 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp c2df77e0-eded-435d-bef8-c151f3b26f5d)
  )
  (fp_circle (center 0 0) (end 4.5 0) (layer "F.SilkS") (width 0.12) (fill none) (tstamp fde410b0-c398-4aca-8278-c3610288e8c0))
  (fp_circle (center 0 0) (end 4.7 0) (layer "F.CrtYd") (width 0.05) (fill none) (tstamp 8fe7ce72-f1fb-4749-8ab2-7ecd3c557e67))
  (pad "1" thru_hole circle (at -2.5 -2.5) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (tstamp 6a6814d5-38db-43ed-8c27-eb8700010790))
  (pad "2" thru_hole circle (at 2.5 2.5) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (tstamp e7f209b6-faaf-4475-b83c-fd0add9a9520))
  (pad "3" thru_hole circle (at -2.5 2.5) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (tstamp 0f9acc25-8b85-47be-9e42-9c3c667a7d2b))
  (pad "4" thru_hole circle (at 2.5 -2.5) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (tstamp 74e4d755-2d96-4314-a5da-c1f35203a178))
  (model "${my_additions}/WOM_package.step"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
