(footprint "MORNSUN_B1212S-2WR2" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "MORNSUN DC-DC isolator. Single")
  (attr through_hole)
  (fp_text reference "REF**" (at 0 5) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp cb2a34a4-6774-4004-9823-5b48a332bc75)
  )
  (fp_text value "B1212S-2WR2" (at -0.25 -2) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 650839f4-132c-4ad9-bb74-6504ac3a1f6b)
  )
  (fp_text user "+Vo" (at 5 2.5 90) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 4f1549c4-23be-4984-a5f1-f314537419ee)
  )
  (fp_text user "Vin" (at -7.5 2 90) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 82677359-4c7d-49b7-8eb1-cabfc8d002a9)
  )
  (fp_text user "0V" (at 0 2 90) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp e4dcd986-f68b-4984-a155-1f0f3e0901ba)
  )
  (fp_text user "GND" (at -5 2.5 90) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp fa366cbd-e18d-4bbe-86ef-2cfacad90535)
  )
  (fp_line (start -10 -1) (end 9.75 -1)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 3a765fe6-1058-4fb3-8b70-337036978fac))
  (fp_line (start -10 6.25) (end -10 -1)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a067c484-1194-4f74-8082-d4b49c21d177))
  (fp_line (start 9.75 -1) (end 9.75 6.25)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 48421134-154d-47c3-9404-15a8209af134))
  (fp_line (start 9.75 6.25) (end -10 6.25)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 16faae0b-a0d0-4ae2-be0e-427b8c9ed16a))
  (fp_rect (start -10 -1) (end 9.7 6.2)
    (stroke (width 0.05) (type default)) (fill none) (layer "F.CrtYd") (tstamp 55d73ae2-ce36-4d7a-b777-a1a9694a1384))
  (fp_rect (start -10 -1) (end 9.7 6.2)
    (stroke (width 0.1) (type default)) (fill none) (layer "F.Fab") (tstamp 0df4fe57-0704-4a28-b8c5-14adae07951b))
  (pad "1" thru_hole circle (at -7.5 0) (size 1.778 1.778) (drill 1.016) (layers "*.Cu" "*.Mask") (tstamp 2b06d8fe-ac9a-4e59-9535-13e6facb2948))
  (pad "2" thru_hole circle (at -5 0) (size 1.778 1.778) (drill 1.016) (layers "*.Cu" "*.Mask") (tstamp ba3bef22-150a-4ded-8ff0-4f921ef9b400))
  (pad "4" thru_hole circle (at 0 0) (size 1.778 1.778) (drill 1.016) (layers "*.Cu" "*.Mask") (tstamp 32893100-21a1-48d4-845d-c938ab115b62))
  (pad "6" thru_hole circle (at 5 0) (size 1.778 1.778) (drill 1.016) (layers "*.Cu" "*.Mask") (tstamp 167cbe78-bf55-4581-9d93-bc243587bf60))
  (model "$(my_additions)/MORNSUN_BxxxxS-2WR2.step"
    (offset (xyz -9.85 -6.15 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
