(footprint "Shunt_L20_H17_D2.5" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "Wire shunt 20mm length, 17mm height, 2.5mm thick")
  (tags "shunt")
  (attr through_hole)
  (fp_text reference "REF**" (at 0 -1 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp b1d3296f-7acf-49aa-a23d-a76559c69e9d)
  )
  (fp_text value "Shunt_L20_H17_D2.5" (at -0.2 3.5 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp e538c55a-66d5-4add-b4fc-b94f6aa46308)
  )
  (fp_text user "${REFERENCE}" (at -0.1 -1.1 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 4285611e-75a0-42ef-bdd9-b8c6b3a5ea8d)
  )
  (fp_line (start -6.8 0) (end 6.8 0)
    (stroke (width 0.12) (type dash)) (layer "F.SilkS") (tstamp 84dbe2bd-4e7e-4182-8835-c0086b1a83c0))
  (fp_circle (center -10 0) (end -6.8 0)
    (stroke (width 0.12) (type default)) (fill none) (layer "F.SilkS") (tstamp 0b3f2900-fcd8-45d6-a79c-78e433095a4d))
  (fp_circle (center 10 0) (end 13.2 0)
    (stroke (width 0.12) (type default)) (fill none) (layer "F.SilkS") (tstamp 55938bf3-b27a-4815-a606-7dd477ded6ed))
  (fp_circle (center -10 0) (end -6.5 0)
    (stroke (width 0.12) (type default)) (fill none) (layer "F.CrtYd") (tstamp 21b9fcc7-b954-4721-9b05-333cb0b9b3b2))
  (fp_circle (center 10 0) (end 13.5 0)
    (stroke (width 0.12) (type default)) (fill none) (layer "F.CrtYd") (tstamp c811444e-afb8-4353-8a6f-f24b50b4372b))
  (fp_line (start -7 0) (end 7 0)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 72b4731d-03a5-4492-9639-42b625a21a95))
  (fp_circle (center -10 0) (end -7 0)
    (stroke (width 0.1) (type default)) (fill none) (layer "F.Fab") (tstamp 74cea6f2-9eec-4826-9dca-b3520e8dbcbb))
  (fp_circle (center 10 0) (end 13 0)
    (stroke (width 0.1) (type default)) (fill none) (layer "F.Fab") (tstamp bf58b722-d150-4289-9f9a-e291bcc93b6b))
  (pad "1" thru_hole circle (at -10 0) (size 5.7 5.7) (drill 2.7) (layers "*.Cu" "*.Mask") (tstamp 642bda1a-f6a1-4c89-922d-3ddfc3c41273))
  (pad "2" thru_hole circle (at 10 0) (size 5.7 5.7) (drill 2.7) (layers "*.Cu" "*.Mask") (tstamp ab3a64fc-8f76-4f18-a2c5-3a36e5680383))
  (model "${my_additions}/Shunt_L20_H17_D2.5.step"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
