(footprint "Transform_D_26.9_14.7_11.2_one_coil_v3_Vertical" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "Transformer on a toroidal core D26.9/14.7/11.2 one coil Horizontal")
  (tags "transformer, toroidal")
  (attr through_hole)
  (fp_text reference "REF**" (at -6.2 -14.8) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify left))
    (tstamp 24e67e86-dfbe-4e5c-bc34-e48aa0ad80ed)
  )
  (fp_text value "Transform_D_26.9_14.7_11.2_one_coil_v3_Vertical" (at 9.2 0 90 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp a66e89f7-244a-48df-a0ce-c24530f40c45)
  )
  (fp_text user "${REFERENCE}" (at 0 -0.1 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 3a022eb6-748d-44d9-9d78-1f97a1218823)
  )
  (fp_line (start -6 -14) (end -6 0.5)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 3f5ffc98-bc3f-4d07-9b06-197415039ee6))
  (fp_line (start -6 5.1) (end -6 14)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 69516256-8841-4024-b55b-15429976ccb0))
  (fp_line (start -6 14) (end 6 14)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp c2f5e05b-2d9d-4873-966b-d2d1658397c1))
  (fp_line (start 6 -14) (end -6 -14)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 11d3a7fe-3390-432a-9f20-e2aee02704cc))
  (fp_line (start 6 -5.1) (end 6 -14)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 87172a91-91ed-4277-8f50-556896905ebc))
  (fp_line (start 6 14) (end 6 -0.5)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp f9edb1e7-8ba0-45b0-b0db-5ce9b471971c))
  (fp_rect (start -8 -16) (end 8 16)
    (stroke (width 0.12) (type default)) (fill none) (layer "F.CrtYd") (tstamp 14a13a5a-ce3b-4a97-b60f-bfee70bd89d2))
  (fp_rect (start -5.9 -13.9) (end 5.9 13.9)
    (stroke (width 0.1) (type default)) (fill none) (layer "F.Fab") (tstamp fb7b235d-8632-48e3-a667-04d1bcb49d04))
  (pad "1" thru_hole circle (at 6.5 -2.8) (size 4 4) (drill 2) (layers "*.Cu" "*.Mask") (tstamp 9b089a06-6942-4750-9e58-c020a7366b9d))
  (pad "2" thru_hole circle (at -6.5 2.8) (size 4 4) (drill 2) (layers "*.Cu" "*.Mask") (tstamp b70d2c14-8515-4d01-84e7-2f05b819a57a))
  (model "${my_additions}/Tor_core_D_26.9_14.7_11.2.step"
    (offset (xyz 5.5 0 15.5))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 90 0))
  )
)
