(footprint "Transform_D_26.9_14.7_11.2_one_coil_Horizontal" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "Transformer on a toroidal core D26.9/14.7/11.2 one coil Horizontal")
  (tags "transformer, toroidal")
  (attr through_hole)
  (fp_text reference "REF**" (at 0 -14.6) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 24e67e86-dfbe-4e5c-bc34-e48aa0ad80ed)
  )
  (fp_text value "Transform_D_26.9_14.7_11.2_one_coil_Horizontal" (at 0 14.6 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp a66e89f7-244a-48df-a0ce-c24530f40c45)
  )
  (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 3a022eb6-748d-44d9-9d78-1f97a1218823)
  )
  (fp_circle (center 0 0) (end 7.2 0)
    (stroke (width 0.12) (type default)) (fill none) (layer "F.SilkS") (tstamp 72ef4589-73c4-44db-949c-459a3155b2dc))
  (fp_circle (center 0 0) (end 13.8 0)
    (stroke (width 0.12) (type default)) (fill none) (layer "F.SilkS") (tstamp 03c6b427-63d8-418c-846e-0fb8110d697f))
  (fp_circle (center 0 0) (end 5.2 0)
    (stroke (width 0.12) (type default)) (fill none) (layer "F.CrtYd") (tstamp 74dad465-2d4d-4ed0-9ad6-6b34daae5202))
  (fp_circle (center 0 0) (end 15.5 0)
    (stroke (width 0.12) (type default)) (fill none) (layer "F.CrtYd") (tstamp 48d439df-53d9-438f-8f6a-044d29c7dcee))
  (fp_circle (center 0 0) (end 7.4 0)
    (stroke (width 0.1) (type default)) (fill none) (layer "F.Fab") (tstamp b9d5e82d-3e74-42c3-9ef6-2e7b041ba3b7))
  (fp_circle (center 0 0) (end 13.4 0)
    (stroke (width 0.1) (type default)) (fill none) (layer "F.Fab") (tstamp 4b6897c7-45f1-4a37-91ad-543d12d0cc1f))
  (pad "1" thru_hole circle (at -4.2 -2.8) (size 4 4) (drill 2) (layers "*.Cu" "*.Mask") (tstamp 9b089a06-6942-4750-9e58-c020a7366b9d))
  (pad "2" thru_hole circle (at -4.2 2.8) (size 4 4) (drill 2) (layers "*.Cu" "*.Mask") (tstamp b70d2c14-8515-4d01-84e7-2f05b819a57a))
  (model "${my_additions}/Tor_core_D_26.9_14.7_11.2.step"
    (offset (xyz 0 0 2))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
