(footprint "Transform_D40_25_7.5_two_coils_v2_Horizontal" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "Transformer on a toroidal core D40/25/7.5 two coils Horizontal")
  (tags "transformer, toroidal")
  (attr through_hole)
  (fp_text reference "REF**" (at 0 -21.2) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp e49933cc-3b8a-494d-a909-c1a3e4dd8f32)
  )
  (fp_text value "Transform_D40_25_7.5_two_coils_v2_Horizontal" (at -0.1 1.9 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 47de6b45-9ab8-4413-a75f-038cd66d5f0e)
  )
  (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 27aa2411-e45e-4fe0-9cc1-28eabc7387e6)
  )
  (fp_circle (center 0 0) (end 12.3 0)
    (stroke (width 0.12) (type default)) (fill none) (layer "F.SilkS") (tstamp b15cd7e4-6853-46b0-8313-65fa30b5a618))
  (fp_circle (center 0 0) (end 20.2 0)
    (stroke (width 0.12) (type default)) (fill none) (layer "F.SilkS") (tstamp 4b5c2a27-53fd-430b-958d-a4adef589174))
  (fp_circle (center 0 0) (end 23.5 0)
    (stroke (width 0.05) (type default)) (fill none) (layer "F.CrtYd") (tstamp 78c0f002-5416-40d2-a4aa-67129b82cfb7))
  (fp_circle (center 0 0) (end 12.5 0)
    (stroke (width 0.1) (type default)) (fill none) (layer "F.Fab") (tstamp 8029da0e-41c0-483e-9055-3c15d0577bfb))
  (fp_circle (center 0 0) (end 20 0)
    (stroke (width 0.1) (type default)) (fill none) (layer "F.Fab") (tstamp 9f164ee6-8fae-48fc-9656-0f1a3a72f669))
  (pad "1" thru_hole circle (at -6 -3.5) (size 4.6 4.6) (drill 2.6) (layers "*.Cu" "*.Mask") (tstamp c4272bc9-1703-4cc0-80cf-e8f60d75d254))
  (pad "2" thru_hole circle (at -18 -15) (size 5.6 5.6) (drill 3.6) (layers "*.Cu" "*.Mask") (tstamp 638e581d-8031-4527-9d81-182aeef4238e))
  (pad "3" thru_hole circle (at 6 -3.5) (size 4.6 4.6) (drill 2.6) (layers "*.Cu" "*.Mask") (tstamp b11602a0-e568-4e0e-932a-0de04f1981f9))
  (pad "4" thru_hole circle (at 6 3.5) (size 4.1 4.1) (drill 2.1) (layers "*.Cu" "*.Mask") (tstamp e9108472-86d7-4499-813d-95d6a5e19492))
  (pad "5" thru_hole circle (at 18 -15) (size 4.6 4.6) (drill 2.6) (layers "*.Cu" "*.Mask") (tstamp 0a252f1c-4338-4c20-9969-05d06148e8ae))
  (pad "6" thru_hole circle (at -6 3.5) (size 4.1 4.1) (drill 2.1) (layers "*.Cu" "*.Mask") (tstamp 23af53e9-21a9-40a2-b74d-060dca4ccea2))
  (model "${my_additions}/Tor_core_Ferrite_D_40_25_7.5_no_coil.step"
    (offset (xyz 0 0 3.6))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
