(module Mc_SWD_conn_programmer_side (layer F.Cu) (tedit 61AE03C6)
  (descr "McFLY's STM32 SWD connector")
  (tags "swd, stm32")
  (fp_text reference SWD (at 0 -2.7) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value Mc_SWD_conn_programmer_side (at 0.1 2.3) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (pad 1 thru_hole circle (at 2.54 -1.27) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "" thru_hole circle (at 4.4 0) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask))
  (pad "" thru_hole circle (at -4.6 1) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask))
  (pad "" thru_hole circle (at -4.6 -1) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at 2.54 1.27) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 3 thru_hole circle (at 0 -1.27) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 4 thru_hole circle (at 0 1.27) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 5 thru_hole circle (at -2.54 -1.27) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 6 thru_hole circle (at -2.54 1.27) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
)
