(footprint "D_SOD-123_with_D_symbol"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "SOD-123")
	(tags "SOD-123")
	(property "Reference" "REF**"
		(at 0 -2 0)
		(layer "F.SilkS")
		(uuid "5c813cbc-84b5-45a4-a0aa-35d3573110db")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "D_SOD-123_with_D_symbol"
		(at 0 2.1 0)
		(layer "F.Fab")
		(uuid "12459980-93ec-4d14-a5d8-25465bd8b01f")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "9df2fb6c-9a01-450c-8dda-024b1c6ddfcc")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "434b35bb-86e7-4a80-b86a-8dfd526da733")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -2.36 -1)
		(end -2.36 1)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "de699020-a29a-4525-a22d-28ad5ded289c")
	)
	(fp_line
		(start -2.36 -1)
		(end 1.65 -1)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "e1b647a2-f10b-41c9-a10d-290cc557cf1b")
	)
	(fp_line
		(start -2.36 1)
		(end 1.65 1)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "bb8e1113-3a33-4b8a-8d4d-dc28453c23b3")
	)
	(fp_line
		(start -0.4 -0.5)
		(end -0.4 0.5)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "28b86e7f-597a-4010-a75a-8c5ad633c5eb")
	)
	(fp_line
		(start -0.4 0)
		(end 0.3 -0.5)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "e9a64f33-e176-4b1b-a560-8635e9279650")
	)
	(fp_line
		(start 0.3 -0.5)
		(end 0.3 0.5)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "65575d8b-edee-4c1c-8329-2d38753f0c32")
	)
	(fp_line
		(start 0.3 0.5)
		(end -0.4 0)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "72d08ea2-c825-409c-a886-d760e228af4e")
	)
	(fp_line
		(start -2.35 -1.15)
		(end -2.35 1.15)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "f234f584-a276-4f4c-b983-7f290a1e5747")
	)
	(fp_line
		(start -2.35 -1.15)
		(end 2.35 -1.15)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "4aacff46-a0e4-4a7e-adc9-4cb9bcd268bd")
	)
	(fp_line
		(start 2.35 -1.15)
		(end 2.35 1.15)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "f57b8828-8e33-4d6a-ba4b-817e53acd1da")
	)
	(fp_line
		(start 2.35 1.15)
		(end -2.35 1.15)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "277b3168-086d-4feb-9ab8-026e88452a58")
	)
	(fp_line
		(start -1.4 -0.9)
		(end 1.4 -0.9)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "4ad4e92b-9b64-4eed-8c4b-d96097a88e61")
	)
	(fp_line
		(start -1.4 0.9)
		(end -1.4 -0.9)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "1ac565ca-970b-44d3-9087-59b04ab60eae")
	)
	(fp_line
		(start -0.75 0)
		(end -0.35 0)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "46dc275b-0899-4d0d-8713-b622e0c22f0e")
	)
	(fp_line
		(start -0.35 0)
		(end -0.35 -0.55)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "9b27c55d-1944-4b36-b982-eb719a46d948")
	)
	(fp_line
		(start -0.35 0)
		(end -0.35 0.55)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "68f6cd3c-fdce-44a9-af86-78cf47501eda")
	)
	(fp_line
		(start -0.35 0)
		(end 0.25 -0.4)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "e7535fdf-c98f-460e-b3e7-c5c3c78dc09f")
	)
	(fp_line
		(start 0.25 -0.4)
		(end 0.25 0.4)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "00b1df15-efaf-4389-b1a8-f9ec8af76c39")
	)
	(fp_line
		(start 0.25 0)
		(end 0.75 0)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "44d78e10-5c1c-4284-ba9c-163e5208ec30")
	)
	(fp_line
		(start 0.25 0.4)
		(end -0.35 0)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "c82b3165-5533-40f3-a703-e13e1a64873f")
	)
	(fp_line
		(start 1.4 -0.9)
		(end 1.4 0.9)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "c36e9a65-0388-45d7-9b3b-1648a22d40d4")
	)
	(fp_line
		(start 1.4 0.9)
		(end -1.4 0.9)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "3ea8d381-2884-4493-a631-0d00c072c3e5")
	)
	(fp_text user "${REFERENCE}"
		(at 0 -2 0)
		(layer "F.Fab")
		(uuid "4ef1dce9-e176-4a2e-8fb0-c36ec2740b29")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd roundrect
		(at -1.65 0)
		(size 0.9 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "8ca7cf40-9887-436c-bea9-a303f4626eef")
	)
	(pad "2" smd roundrect
		(at 1.65 0)
		(size 0.9 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "6df6f7bc-2215-4f91-8920-244285a2df55")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
