(footprint "SW_micro_2x4x3.5_angled"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Micro tactile angled button 2x4x3.5mm")
	(tags "1TS003B, TS-1100AAEP, button, micro")
	(property "Reference" "REF**"
		(at -3.5 -0.1 90)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "5f02d20e-d714-4c11-b966-3e343a09c90a")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "1TS003B"
		(at 0 4.2 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "fe26eb7f-af2d-443d-afe2-436484e1b919")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "1e88c19e-ffeb-4f59-acb5-bcac3897663d")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" "Micro tactile angled button 2x4x3.5mm"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "e6f76ac8-8c62-4cc5-b112-fc66264c9ef5")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -2.4 0.2)
		(end -2.4 1.3)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "8bcb2844-3ef1-40f8-9ac5-5ea90622b4e7")
	)
	(fp_line
		(start -2.4 1.3)
		(end -2.2 1.3)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "700f5d7e-8732-4a57-b32f-fddee0c16d71")
	)
	(fp_line
		(start -1.4 -1.3)
		(end 1.4 -1.3)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "839e416e-eea5-45db-a3c5-1d7f59ed38c6")
	)
	(fp_line
		(start -1.2 1.3)
		(end 1.2 1.3)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "fe46a3e6-b238-4242-b0bb-467d024a80f4")
	)
	(fp_line
		(start 2.2 1.3)
		(end 2.4 1.3)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "ab2e0c7b-96b9-46f1-ab00-9fd82d4b9e67")
	)
	(fp_line
		(start 2.4 1.3)
		(end 2.4 0.2)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "77914bfb-8070-415c-a81a-ac65e7e94bfa")
	)
	(fp_rect
		(start -2.325 -1.2)
		(end 2.325 1.2)
		(stroke
			(width 0.05)
			(type solid)
		)
		(fill no)
		(layer "F.CrtYd")
		(uuid "4eb51e50-9a66-4e95-b89c-478aa866a356")
	)
	(fp_rect
		(start -2.3 -1.2)
		(end 2.3 1.2)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill no)
		(layer "F.Fab")
		(uuid "5ca5a23a-142d-40e1-bcf6-4f6f2c54571e")
	)
	(fp_rect
		(start -1 -2.2)
		(end 1 -1.2)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill no)
		(layer "F.Fab")
		(uuid "4c176b9e-c5c3-4bb7-aba0-2a4e44546c00")
	)
	(fp_text user "${REFERENCE}"
		(at 0.1 2.8 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "f8141b6a-cad1-4c60-ab30-4621404b5fdf")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "" np_thru_hole circle
		(at -0.85 0)
		(size 0.75 0.75)
		(drill 0.75)
		(layers "F&B.Cu" "*.Mask")
		(uuid "82318e2e-f265-4f05-ba34-1c900209db32")
	)
	(pad "" np_thru_hole circle
		(at 0.85 0)
		(size 0.75 0.75)
		(drill 0.75)
		(layers "F&B.Cu" "*.Mask")
		(uuid "492515a2-1206-4e6b-b788-92732bc5cc0d")
	)
	(pad "1" smd rect
		(at -1.7 1.3)
		(size 0.65 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "b714ba55-1fd9-40b8-9604-867cd76642ca")
	)
	(pad "2" smd rect
		(at 1.7 1.3)
		(size 0.65 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "894a3e1e-cad2-4b5d-8490-fb5cd779db29")
	)
	(pad "3" smd custom
		(at -2.325 -0.65)
		(size 0.65 1.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.175 -0.65) (xy 0.725 -0.65) (xy 0.725 0) (xy -0.175 0)
				)
				(width 0)
				(fill yes)
			)
		)
		(uuid "0cbde0a0-86e8-44ef-b5a2-bcfd8b9b19cd")
	)
	(pad "4" smd custom
		(at 2.325 -0.65)
		(size 0.65 1.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.275 -0.65) (xy -0.725 -0.65) (xy -0.725 0) (xy 0.275 0)
				)
				(width 0)
				(fill yes)
			)
		)
		(uuid "0a738c8d-e2b4-49ae-a4e5-3035858c11e9")
	)
	(embedded_fonts no)
	(model "${MY_ADDITIONS}/1TS003B_2x4x3.5.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 -0 -0)
		)
	)
)
