(footprint "Buzzer_5020"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Buzzer 5x5x2mm 2-4v")
	(tags "buzzer 5020")
	(property "Reference" "REF**"
		(at -0.1 -3.5 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "a264eadd-10cf-4ff0-8658-27d2364ef3ec")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "Buzzer_5020"
		(at 0 3.7 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "1e5852f6-08e4-43b0-83c0-67f11c9e1c71")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "45caf661-65b8-42d5-bb47-8e7bb9a593fc")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "52fbf23d-1cc8-4616-bf07-4e3fbc08e86f")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -2.6 -2.6)
		(end 1.6 -2.6)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "39a13777-4699-46ab-a3ad-3c1947f2d605")
	)
	(fp_line
		(start -2.6 0.9)
		(end -2.6 -0.9)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "70d3c1dc-12cb-42e1-af57-d552eb2d1c88")
	)
	(fp_line
		(start -2.6 2.6)
		(end 2.6 2.6)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "8378d8d5-2e37-4fcd-8854-49d23a24ddd2")
	)
	(fp_line
		(start 1.6 -2.6)
		(end 2.6 -1.6)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "b12e9fd9-c568-4d72-b0ab-aeaca64fd758")
	)
	(fp_line
		(start 2.6 -1.6)
		(end 2.6 0.9)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "2fcd4eef-5c1a-4ec5-b854-d6b8e3a15ab6")
	)
	(fp_circle
		(center 0 -1.15)
		(end 0.4 -1.15)
		(stroke
			(width 0.12)
			(type solid)
		)
		(fill no)
		(layer "F.SilkS")
		(uuid "453fb9b1-c76f-4075-80b9-c943970c51d0")
	)
	(fp_rect
		(start -2.8 -2.8)
		(end 2.8 2.8)
		(stroke
			(width 0.12)
			(type solid)
		)
		(fill no)
		(layer "F.CrtYd")
		(uuid "88524f99-ea7c-4275-94c3-0aa0e559ecb1")
	)
	(pad "" smd rect
		(at -2.25 -1.75)
		(size 2.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "56009e6e-6109-476d-8d4a-25f09ba71bf5")
	)
	(pad "1" smd rect
		(at -2.25 1.75)
		(size 2.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "8da527fe-a8dd-46f1-ae83-f28e51920d2d")
	)
	(pad "2" smd rect
		(at 2.25 1.75)
		(size 2.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "ca67c3ac-5c9e-4dcb-8d5d-cf43f80506a2")
	)
	(embedded_fonts no)
	(model "${MY_ADDITIONS}/Buzzer_5020.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
