(footprint "USB-C_Receptable_14P_Vertical"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at -5.1 0 90)
		(layer "F.SilkS")
		(uuid "de101ea3-f6d8-4b8a-b7f9-ffd0a335d66e")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "USB-C_Receptable_14P_Vertical"
		(at 0 2.5 0)
		(layer "F.Fab")
		(uuid "73002f14-9c1d-43f0-b611-e38e6ae0df70")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "7f67c2d4-9dc2-416f-90f0-b2fad968e34a")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "a70d91c3-e30e-4e2e-a543-445865ec4f82")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole)
	(fp_line
		(start -4.3 -1.55)
		(end -4.3 1.55)
		(stroke
			(width 0.15)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "ccb47611-2554-47b6-9f26-d20a7827ef61")
	)
	(fp_line
		(start -4.3 -1.55)
		(end -3.05 -1.55)
		(stroke
			(width 0.15)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "4fa87f3d-d8fa-40a6-a364-7dc0e4883c66")
	)
	(fp_line
		(start -4.3 1.55)
		(end -3.05 1.55)
		(stroke
			(width 0.15)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "3626666b-914d-4642-b0f3-6116b268411b")
	)
	(fp_line
		(start -0.95 -1.55)
		(end 0.95 -1.55)
		(stroke
			(width 0.15)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "87d493e2-a305-4bd2-88e5-c5af4e210854")
	)
	(fp_line
		(start -0.95 1.55)
		(end 0.95 1.55)
		(stroke
			(width 0.15)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "fff1362e-60c2-4240-a1eb-5d0a5c04afa8")
	)
	(fp_line
		(start 3.05 1.55)
		(end 4.3 1.55)
		(stroke
			(width 0.15)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "824a64a0-88ab-4cc8-b835-b0d5e76dd4cd")
	)
	(fp_line
		(start 4.3 -1.55)
		(end 3.05 -1.55)
		(stroke
			(width 0.15)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "cd00262d-ea9f-41cd-91d0-28744df5de9b")
	)
	(fp_line
		(start 4.3 1.55)
		(end 4.3 -1.55)
		(stroke
			(width 0.15)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "5889fdc2-902f-457c-8c2e-570f9926d260")
	)
	(fp_line
		(start -4.25 1.5)
		(end -4.25 -1.5)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "9725267c-a02b-47df-ae4c-68ad2478e54c")
	)
	(fp_line
		(start -3 -2.35)
		(end -3 -1.5)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "3eba1cba-b076-4161-8b94-9daf95bacaef")
	)
	(fp_line
		(start -3 -1.5)
		(end -4.25 -1.5)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "973fb825-6758-46c1-8ab8-3f08b0f4696b")
	)
	(fp_line
		(start -3 1.5)
		(end -4.25 1.5)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "7cdd3235-6639-428d-9979-a1145ada5a65")
	)
	(fp_line
		(start -3 1.5)
		(end -3 2.35)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "691b3001-7a77-4d5a-97a5-b83f5467ff93")
	)
	(fp_line
		(start -3 2.35)
		(end -1 2.35)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "5d0596c4-d30a-40ad-b46f-0b54a31dc842")
	)
	(fp_line
		(start -1 -2.35)
		(end -3 -2.35)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "4e558c99-f885-4c23-8986-9c03f754b110")
	)
	(fp_line
		(start -1 -1.5)
		(end -1 -2.35)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "cae5bb69-1329-437f-8b98-65f931a0c708")
	)
	(fp_line
		(start -1 2.35)
		(end -1 1.5)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "548cfc41-ecc7-4351-b554-d114f0f2daa3")
	)
	(fp_line
		(start 1 -2.35)
		(end 1 -1.5)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "1763c1aa-714e-4e58-829f-cdc018055960")
	)
	(fp_line
		(start 1 -1.5)
		(end -1 -1.5)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "f35f442b-ab94-4c36-af4d-382cbd028131")
	)
	(fp_line
		(start 1 1.5)
		(end -1 1.5)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "00909ec4-1b85-4c62-8b91-fcdf1146813d")
	)
	(fp_line
		(start 1 1.5)
		(end 1 2.35)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "11753f38-b373-4cbe-880d-ee665db2f20d")
	)
	(fp_line
		(start 1 2.35)
		(end 3 2.35)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "21dd2f90-116a-43bc-a204-41e3d25b2fa2")
	)
	(fp_line
		(start 3 -2.35)
		(end 1 -2.35)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "a10fb1ca-a06f-49ba-bcd3-75e6a2307e63")
	)
	(fp_line
		(start 3 -1.5)
		(end 3 -2.35)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "2516bdcb-a3ee-4bf0-b22f-6678b9edc7b1")
	)
	(fp_line
		(start 3 2.35)
		(end 3 1.5)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "d08e393b-de7f-4929-8b2b-c383acf67ae0")
	)
	(fp_line
		(start 4.25 -1.5)
		(end 3 -1.5)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "9b543a47-295b-4582-8363-123e50119526")
	)
	(fp_line
		(start 4.25 -1.5)
		(end 4.25 1.5)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "3c3e045d-2166-48ae-86de-0f0b0dee110f")
	)
	(fp_line
		(start 4.25 1.5)
		(end 3 1.5)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "ea06fa1f-556f-457b-890b-d5ee6515a2d1")
	)
	(fp_rect
		(start -4.2 -1.45)
		(end 4.2 1.45)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill no)
		(layer "F.Fab")
		(uuid "5d52120a-aab8-461f-8e82-beaf8edd09ce")
	)
	(fp_text user "${REFERENCE}"
		(at 0 4 0)
		(layer "F.Fab")
		(uuid "cd44d10b-3d55-4cab-a793-793f066c0078")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "A1" thru_hole oval
		(at -3.25 -0.7)
		(size 0.7 0.9)
		(drill 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "348ba6af-a29f-4833-acb0-400162619f35")
	)
	(pad "A4" thru_hole oval
		(at -2.3 -0.7)
		(size 0.7 0.9)
		(drill 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "bd1ad288-29fa-4a5a-8133-b52df1dfbe4f")
	)
	(pad "A5" thru_hole oval
		(at -1.35 -0.7)
		(size 0.7 0.9)
		(drill 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "8f63282a-ea12-4115-abb0-0fd6431e3088")
	)
	(pad "A6" thru_hole oval
		(at -0.45 -0.7)
		(size 0.7 0.9)
		(drill 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "48a56ec7-b032-4ef9-a1f0-362722d18a64")
	)
	(pad "A7" thru_hole oval
		(at 0.45 -0.7)
		(size 0.7 0.9)
		(drill 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "4af3a456-5034-42af-b3de-f4c1af94b3bd")
	)
	(pad "A9" thru_hole oval
		(at 2.3 -0.7)
		(size 0.7 0.9)
		(drill 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "c54afb7a-f3ba-4c00-83e3-e4739daf367d")
	)
	(pad "A12" thru_hole oval
		(at 3.25 -0.7)
		(size 0.7 0.9)
		(drill 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "072ab194-ca89-4a8a-a10d-5ce27d6d0aff")
	)
	(pad "B1" thru_hole oval
		(at 3.25 0.7)
		(size 0.7 0.9)
		(drill 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "7086f4dd-1b56-4a4a-81e1-4ef1d8f654f5")
	)
	(pad "B4" thru_hole oval
		(at 2.3 0.7)
		(size 0.7 0.9)
		(drill 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "405f3927-a1ad-40f8-b791-22b205b73d25")
	)
	(pad "B5" thru_hole oval
		(at 1.35 0.7)
		(size 0.7 0.9)
		(drill 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "aa6124c6-cb0b-48bc-9085-70b062bc7aaf")
	)
	(pad "B6" thru_hole oval
		(at 0.45 0.7)
		(size 0.7 0.9)
		(drill 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "67a626cc-cb45-4893-b0b2-6bf167c84e51")
	)
	(pad "B7" thru_hole oval
		(at -0.45 0.7)
		(size 0.7 0.9)
		(drill 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "adc8ed10-6887-4b66-b69a-1266e6740d29")
	)
	(pad "B9" thru_hole oval
		(at -2.3 0.7)
		(size 0.7 0.9)
		(drill 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "63895f0c-6a0e-42cf-9ceb-ac084fe356b0")
	)
	(pad "B12" thru_hole oval
		(at -3.25 0.7)
		(size 0.7 0.9)
		(drill 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "074fb31d-f92c-4463-bdab-a3811a66f4b2")
	)
	(pad "S1" thru_hole oval
		(at -2 -1.93)
		(size 2 0.9)
		(drill oval 1.6 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "218260b8-d425-4aa7-bb66-f4d42dbb1e4d")
	)
	(pad "S1" thru_hole oval
		(at -2 1.93)
		(size 2 0.9)
		(drill oval 1.6 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "9a2b1bfd-74fa-4d7b-88cc-c1b43377f9d0")
	)
	(pad "S1" thru_hole oval
		(at 2 -1.93)
		(size 2 0.9)
		(drill oval 1.6 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "be9feb4b-4604-4579-94a9-e41b809eea3a")
	)
	(pad "S1" thru_hole oval
		(at 2 1.93)
		(size 2 0.9)
		(drill oval 1.6 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "6e86d7d9-b121-4fa4-b61b-37cb07ccdce9")
	)
	(embedded_fonts no)
	(model "${MY_ADDITIONS}/TYPE-C-14-vertical_H-10mm.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
