(footprint "SolderJumper-2_Open_TrianglePad_smaller"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "SMD Solder Jumper, 1x1.5mm Triangular Pads, 0.3mm gap, open")
	(tags "solder jumper open")
	(property "Reference" "REF**"
		(at 0 -1.4 0)
		(layer "F.SilkS")
		(uuid "b9c83bb8-4f46-406b-bb8c-95f6709eb55c")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "SolderJumper-2_Open_TrianglePad_smaller"
		(at 0 1.9 0)
		(layer "F.Fab")
		(uuid "a752f8c1-d50d-4fd4-83d1-e4b7c9358d47")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "31843f8d-2ed7-402b-8724-a9da05b0c3d7")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "117c75e5-c34c-4292-ab72-83f4e5c3a290")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(zone_connect 1)
	(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
	(fp_rect
		(start -1.075 -0.55)
		(end 1.075 0.55)
		(stroke
			(width 0)
			(type default)
		)
		(fill yes)
		(layer "F.Mask")
		(uuid "de436a83-4adc-400f-9a0d-06fb2990be49")
	)
	(fp_rect
		(start -1.225 -0.7)
		(end 1.225 0.7)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill no)
		(layer "F.CrtYd")
		(uuid "e0d12e2c-18f8-4e41-a323-1ad76f006d6d")
	)
	(pad "1" smd custom
		(at -0.875 0)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask")
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy 1 0) (xy 0.633334 0.55) (xy -0.2 0.55) (xy -0.2 -0.55) (xy 0.633334 -0.55)
				)
				(width 0)
				(fill yes)
			)
		)
		(uuid "b69c9f40-8973-419c-b2c0-dbebaca6e371")
	)
	(pad "2" smd custom
		(at 0.575 0)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask")
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.5 0.55) (xy -0.516666 0.55) (xy -0.15 0) (xy -0.516666 -0.55) (xy 0.5 -0.55)
				)
				(width 0)
				(fill yes)
			)
		)
		(uuid "8970f70d-502a-401e-b938-b9f4e820a1e7")
	)
	(embedded_fonts no)
)
