(footprint "TCT40-16T"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Ultrasonic transmitter")
	(property "Reference" "REF**"
		(at 0 -9 0)
		(layer "F.SilkS")
		(uuid "a0e82f31-0d4f-4de3-978e-1413e1850eca")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "TCT40-16T"
		(at 0 4.95 0)
		(layer "F.Fab")
		(uuid "4190ec76-95b1-4e51-ad4e-4fa27adabf9d")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "fc15f49f-8d11-4028-b010-79caedc512e5")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" "Ultrasonic transmitter"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "77356c7f-095b-4ba3-8932-f1bad57c0727")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole)
	(fp_circle
		(center 0 0)
		(end 8.1 0)
		(stroke
			(width 0.15)
			(type default)
		)
		(fill no)
		(layer "F.SilkS")
		(uuid "e06c8c67-8f97-4744-8a06-77aa85a00c39")
	)
	(fp_circle
		(center 0 0)
		(end 8 0)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill no)
		(layer "F.CrtYd")
		(uuid "f6692777-7596-4aaf-bb19-f4fd9c490293")
	)
	(fp_circle
		(center 0 0)
		(end 8 0)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill no)
		(layer "F.Fab")
		(uuid "5a3c5e39-754f-42f7-91a7-ae8910f9fa32")
	)
	(fp_text user "+"
		(at -5 2 0)
		(layer "F.SilkS")
		(uuid "cebdfb29-7f89-49c2-b1c4-ee38c8a2166c")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(fp_text user "${REFERENCE}"
		(at 0 3.45 0)
		(layer "F.Fab")
		(uuid "d018c55c-29b2-472e-918c-58b81fb43d4d")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" thru_hole circle
		(at -5 0)
		(size 2.8 2.8)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "68801684-88a4-4626-8d2e-25b729552aa1")
	)
	(pad "2" thru_hole circle
		(at 5 0)
		(size 2.8 2.8)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "6f2baa81-3a4f-4954-96e8-eaa51400c602")
	)
	(embedded_fonts no)
	(model "${MY_ADDITIONS}/tct40-16t.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
