(footprint "SIM800L-module"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "SIM800L GSM module")
	(tags "SIM800, GMS, module,")
	(property "Reference" "REF**"
		(at -12.6 -12.5 0)
		(layer "F.SilkS")
		(uuid "2b162358-e413-40aa-b0d2-bb19b2a8994d")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
			(justify left)
		)
	)
	(property "Value" "SIM800L-module"
		(at 0 2.7 0)
		(layer "F.Fab")
		(uuid "c2a4987f-ef9b-4307-8cd0-937b4396e4a7")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "e9c19fdc-95b1-49bd-bca3-875fe040f11c")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "0e2ea4b8-fafb-45a6-80ac-bb63a189849e")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole)
	(fp_rect
		(start -12.6 -11.6)
		(end 12.6 11.6)
		(stroke
			(width 0.15)
			(type default)
		)
		(fill no)
		(layer "F.SilkS")
		(uuid "d3098dd8-37fa-46d5-96ab-ea0a62022f66")
	)
	(fp_rect
		(start -12.5 -11.5)
		(end 12.5 11.5)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill no)
		(layer "F.CrtYd")
		(uuid "7f444351-2cca-4a46-9264-1c163ac24cd0")
	)
	(fp_line
		(start -4.1 -17.6)
		(end 3.9 -17.6)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "9fc57228-0d09-4efc-9bc4-f6d7fde8705c")
	)
	(fp_line
		(start -4.1 -11.4)
		(end -4.1 -17.6)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "f90e06f0-3d90-4739-82dd-f6b2fc78034e")
	)
	(fp_line
		(start -0.3 -12.9)
		(end 0 -11.9)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "d26c01c2-755f-44ec-b5ff-77f00b80d567")
	)
	(fp_line
		(start 0 -12.9)
		(end 0 -15.2)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "75cc5d12-d490-4405-b36f-491c1de5d263")
	)
	(fp_line
		(start 0 -11.9)
		(end 0.3 -12.9)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "0b839e70-4cdf-4764-936c-0269ca4aa5ec")
	)
	(fp_line
		(start 0.3 -12.9)
		(end -0.3 -12.9)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "39554a2f-18fa-482f-8fa9-b3801c7538fc")
	)
	(fp_line
		(start 3.9 -17.6)
		(end 3.9 -11.4)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "0576a317-3886-494a-acad-b1fe2d1aaec5")
	)
	(fp_rect
		(start -12.4 -11.4)
		(end 12.4 11.4)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill no)
		(layer "F.Fab")
		(uuid "ed76da88-12a6-4512-86ad-3587bd05f523")
	)
	(fp_rect
		(start -8 -5.1)
		(end 8 10.2)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill no)
		(layer "F.Fab")
		(uuid "cabcf77b-caa7-4a3b-a81a-a958465f56fd")
	)
	(fp_arc
		(start 2.9 -11.4)
		(mid 0 -8.5)
		(end -2.9 -11.4)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "3f977e38-b756-45a3-884c-15f22cbe8d0b")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
		(uuid "60c58827-6aae-46dc-a86c-3ccb1f2ea07a")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(fp_text user "SIM"
		(at 0 -15.7 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "bbdc9a4c-7935-4f5c-9dd9-ac9e2a8e624f")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
			(justify bottom)
		)
	)
	(pad "2" thru_hole circle
		(at -11 -4.16 90)
		(size 2 2)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "4de7d336-be68-4754-b34f-23ab10153335")
	)
	(pad "3" thru_hole circle
		(at -11 -1.62 90)
		(size 2 2)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "4dc137eb-5aa0-4538-9037-31253cf83aff")
	)
	(pad "4" thru_hole circle
		(at -11 0.92 90)
		(size 2 2)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "743ef3e3-2347-48d7-a1b8-388084fcabda")
	)
	(pad "5" thru_hole circle
		(at -11 3.46 90)
		(size 2 2)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "371f29a0-80cc-48ce-8120-4ce423fc1311")
	)
	(pad "6" thru_hole circle
		(at -11 6 90)
		(size 2 2)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "cb9fda53-0acd-4c4b-9048-79bc741b426e")
	)
	(pad "7" thru_hole circle
		(at 11 8.5 90)
		(size 2 2)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "de97df00-6462-4419-82f9-aebcd4ba2267")
	)
	(pad "8" thru_hole circle
		(at 11 5.96 90)
		(size 2 2)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "7adeaa13-1e79-4825-bc9b-37f97bcf67f5")
	)
	(pad "9" thru_hole circle
		(at 11 3.42 90)
		(size 2 2)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "f15ccc1b-8464-428e-bc6f-7ef07fe6b020")
	)
	(pad "10" thru_hole circle
		(at 11 0.88 90)
		(size 2 2)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "22e55f03-7122-4df2-a6b2-7092fea41094")
	)
	(pad "11" thru_hole circle
		(at 11 -1.66 90)
		(size 2 2)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "da23fc14-55e7-4c8e-9e4f-cfcfd2a8c1bd")
	)
	(pad "12" thru_hole circle
		(at 11 -4.2 90)
		(size 2 2)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "b3ff6056-06b5-44c1-9252-0d2a34323f25")
	)
	(embedded_fonts no)
	(model "${MY_ADDITIONS}/SIM800L.step"
		(offset
			(xyz 0 0 2.5)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
