(footprint "BNC-KE_22.5mm_long"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "BNC female PCB mount 4 pin straight chassis connector http://www.te.com/usa-en/product-1-1478204-0.html")
	(tags "BNC female PCB mount 4 pin straight chassis connector ")
	(property "Reference" "REF**"
		(at -0.25 -6.25 0)
		(layer "F.SilkS")
		(uuid "3a6ff247-253c-46be-bf30-139c658c06f9")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "BNC-KE_22.5mm_long"
		(at 0 6.5 0)
		(layer "F.Fab")
		(uuid "bb0e2cba-5c99-48d6-8e5e-97a69e16a3cd")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "76516dde-152b-465e-9045-cfd7bc2563df")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "05fc97f5-4a4e-4c36-8c3a-f15d1f1bffb8")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole)
	(fp_arc
		(start -4.9 2.5)
		(mid -5.500909 0)
		(end -4.9 -2.5)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "2c912a0b-2f09-4208-85ae-00c0baa3721d")
	)
	(fp_arc
		(start -2.5 -4.9)
		(mid 0 -5.500909)
		(end 2.5 -4.9)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "0e0eb948-47b3-4c42-bddc-0d0de9019f71")
	)
	(fp_arc
		(start 2.5 4.9)
		(mid 0 5.500909)
		(end -2.5 4.9)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "7233b03f-1ef1-47c4-b6ae-f7b38a25f1d9")
	)
	(fp_arc
		(start 4.9 -2.5)
		(mid 5.500909 0)
		(end 4.9 2.5)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "d2558a92-acf9-4fea-bbb6-ee3755eb23e7")
	)
	(fp_line
		(start -5.5 -5.5)
		(end 5.5 -5.5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "8db283cc-f882-4a57-96da-3f857f09b0cc")
	)
	(fp_line
		(start -5.5 5.5)
		(end -5.5 -5.5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "2c72c170-89db-4819-9dcb-1e73e2e1e548")
	)
	(fp_line
		(start 5.5 -5.5)
		(end 5.5 5.5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "6967a5f4-0742-47e4-987c-aeccd5fab0f1")
	)
	(fp_line
		(start 5.5 5.5)
		(end -5.5 5.5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "c282a32f-bbb1-4e82-bdc8-53df2ddff881")
	)
	(fp_circle
		(center 0 0)
		(end 5.5 0)
		(stroke
			(width 0.1)
			(type solid)
		)
		(fill no)
		(layer "F.Fab")
		(uuid "b9aa5c04-7a16-4b74-a6ab-066a7d1d9496")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
		(uuid "a21a3d9c-6c11-4f52-8401-f5259b1d58ca")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 2.8 2.8)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "f0f7bfb4-2033-4ee5-a1c9-e4e5b846ec80")
	)
	(pad "2" thru_hole circle
		(at -3.25 -3.25)
		(size 3.4 3.4)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "553b2698-79f2-4522-9029-f003906cce61")
	)
	(pad "2" thru_hole circle
		(at -3.25 3.25)
		(size 3.4 3.4)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "f21f9418-7d42-4668-9843-8d8fac878198")
	)
	(pad "2" thru_hole circle
		(at 3.25 -3.25)
		(size 3.4 3.4)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "d2cba9ae-5d2e-4ce8-8282-96fe847d4171")
	)
	(pad "2" thru_hole circle
		(at 3.25 3.25)
		(size 3.4 3.4)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "5d1bd656-097b-4603-a789-891bc267ca20")
	)
	(embedded_fonts no)
	(model "${MY_ADDITIONS}/BNC-KE_jack.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
