(footprint "MORNSUN_B1212S-2WR2"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "MORNSUN DC-DC isolator. Single")
	(property "Reference" "REF**"
		(at 0 5 0)
		(layer "F.SilkS")
		(uuid "cb2a34a4-6774-4004-9823-5b48a332bc75")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "B1212S-2WR2"
		(at -0.25 -2 0)
		(layer "F.Fab")
		(uuid "650839f4-132c-4ad9-bb74-6504ac3a1f6b")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "2dfdafd8-3607-4fdd-9122-e5cfddf60153")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "97bd2bbd-eb17-4f03-814a-0aac23abcd11")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole)
	(fp_line
		(start -10 -1)
		(end 9.75 -1)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "3a765fe6-1058-4fb3-8b70-337036978fac")
	)
	(fp_line
		(start -10 6.25)
		(end -10 -1)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "a067c484-1194-4f74-8082-d4b49c21d177")
	)
	(fp_line
		(start 9.75 -1)
		(end 9.75 6.25)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "48421134-154d-47c3-9404-15a8209af134")
	)
	(fp_line
		(start 9.75 6.25)
		(end -10 6.25)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "16faae0b-a0d0-4ae2-be0e-427b8c9ed16a")
	)
	(fp_rect
		(start -10 -1)
		(end 9.7 6.2)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill no)
		(layer "F.CrtYd")
		(uuid "55d73ae2-ce36-4d7a-b777-a1a9694a1384")
	)
	(fp_rect
		(start -10 -1)
		(end 9.7 6.2)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill no)
		(layer "F.Fab")
		(uuid "0df4fe57-0704-4a28-b8c5-14adae07951b")
	)
	(fp_text user "+Vo"
		(at 5 2.5 90)
		(layer "F.SilkS")
		(uuid "4f1549c4-23be-4984-a5f1-f314537419ee")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(fp_text user "Vin"
		(at -7.5 2 90)
		(layer "F.SilkS")
		(uuid "82677359-4c7d-49b7-8eb1-cabfc8d002a9")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(fp_text user "0V"
		(at 0 2 90)
		(layer "F.SilkS")
		(uuid "e4dcd986-f68b-4984-a155-1f0f3e0901ba")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(fp_text user "GND"
		(at -5 2.5 90)
		(layer "F.SilkS")
		(uuid "fa366cbd-e18d-4bbe-86ef-2cfacad90535")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" thru_hole circle
		(at -7.5 0)
		(size 1.778 1.778)
		(drill 1.016)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "2b06d8fe-ac9a-4e59-9535-13e6facb2948")
	)
	(pad "2" thru_hole circle
		(at -5 0)
		(size 1.778 1.778)
		(drill 1.016)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "ba3bef22-150a-4ded-8ff0-4f921ef9b400")
	)
	(pad "4" thru_hole circle
		(at 0 0)
		(size 1.778 1.778)
		(drill 1.016)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "32893100-21a1-48d4-845d-c938ab115b62")
	)
	(pad "6" thru_hole circle
		(at 5 0)
		(size 1.778 1.778)
		(drill 1.016)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "167cbe78-bf55-4581-9d93-bc243587bf60")
	)
	(embedded_fonts no)
	(model "${MY_ADDITIONS}/MORNSUN_BxxxxS-2WR2.step"
		(offset
			(xyz -9.85 -6.15 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
