(footprint "USB_Micro-B_Vertical"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "USB Micro-B receptacle, through-hole, vertical,")
	(tags "usb micro receptacle vertical")
	(property "Reference" "REF**"
		(at 1.3 -2.48 0)
		(layer "F.SilkS")
		(uuid "c6aff463-1363-48b4-b491-2a56b962fcb6")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "USB_Micro-B_Vertical"
		(at 1.3 2.92 0)
		(layer "F.Fab")
		(uuid "248be61f-2fb7-4ca1-95e0-6330332e00b2")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "ee380f09-c3be-4054-bc07-2877b5c6aa78")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "a7da4252-7be6-47ce-b13d-b73a997cb510")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole)
	(fp_line
		(start -2.85 -1.38)
		(end 5.45 -1.38)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "ad65b1c5-de24-4776-b316-9c1683005c96")
	)
	(fp_line
		(start -2.85 -0.905)
		(end -2.85 -1.38)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "9b4c5cd3-40df-4df2-9d94-2cecde43f3c3")
	)
	(fp_line
		(start -2.85 1.345)
		(end -2.85 1.82)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "a32196ef-2ccc-4b7d-b113-0f3497b11066")
	)
	(fp_line
		(start -2.85 1.82)
		(end 5.45 1.82)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "e3bfe556-1451-4579-8605-2a9375eb913e")
	)
	(fp_line
		(start -1 -1.68)
		(end 1 -1.68)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "317f3c24-19a5-4197-8d8d-ae6577a41849")
	)
	(fp_line
		(start 5.45 -1.38)
		(end 5.45 -0.905)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "1750c308-b8b8-416f-9c4c-778e590d3db4")
	)
	(fp_line
		(start 5.45 1.82)
		(end 5.45 1.345)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "af086fd3-2b7c-49f5-bbe7-f7af734245f8")
	)
	(fp_line
		(start -3.2 -1.73)
		(end -3.2 2.17)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "ae3ae96a-2368-4626-9355-aa7fbd95821d")
	)
	(fp_line
		(start -3.2 2.17)
		(end 5.8 2.17)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "cf653026-43dd-4e81-8325-9def1d71b262")
	)
	(fp_line
		(start 5.8 -1.73)
		(end -3.2 -1.73)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "a9f3369c-bc0f-4c9c-ae40-8c6331f33180")
	)
	(fp_line
		(start 5.8 2.17)
		(end 5.8 -1.73)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "f24ca52a-a124-4eee-b518-f9bbf35b4b55")
	)
	(fp_line
		(start -2.7 -1.23)
		(end -1 -1.23)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "ff00f0f2-28f2-4c94-8f8a-969dfad604f7")
	)
	(fp_line
		(start -2.7 1.67)
		(end -2.7 -1.23)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "41b6563c-7a6c-4821-93ea-ad07b2c850d8")
	)
	(fp_line
		(start -1 -1.23)
		(end 0 -0.23)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "abba648a-57bf-4331-8895-87417039bb5a")
	)
	(fp_line
		(start 0 -0.23)
		(end 1 -1.23)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "48cc58f9-b051-411b-aa71-169d76701ad3")
	)
	(fp_line
		(start 1 -1.23)
		(end 5.3 -1.23)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "54602339-d83a-4fdc-8059-75d5000ad76e")
	)
	(fp_line
		(start 5.3 -1.23)
		(end 5.3 1.67)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "148d5cc4-b156-433f-9f4e-753b4a7297d4")
	)
	(fp_line
		(start 5.3 1.67)
		(end -2.7 1.67)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "246198e1-6c06-44a7-b391-60f16bc7dbaf")
	)
	(fp_text user "${REFERENCE}"
		(at 1.3 0.22 0)
		(layer "F.Fab")
		(uuid "26318f28-2115-4360-a983-bf4cf7c644da")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 0.84 0.84)
		(drill 0.44)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "5da9cb99-16b4-47e4-bf0f-c34b302dae9c")
	)
	(pad "2" thru_hole circle
		(at 0.65 1)
		(size 0.84 0.84)
		(drill 0.44)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "ef3bee2d-391b-42b2-9695-d2cbc6a51b8c")
	)
	(pad "3" thru_hole circle
		(at 1.3 0)
		(size 0.84 0.84)
		(drill 0.44)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "bb97af1d-6c99-4ea5-b93e-30901724bec1")
	)
	(pad "4" thru_hole circle
		(at 1.95 1)
		(size 0.84 0.84)
		(drill 0.44)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "9b9b7fab-fa4e-4192-bba5-5e24651edf32")
	)
	(pad "5" thru_hole circle
		(at 2.6 0)
		(size 0.84 0.84)
		(drill 0.44)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "6e78b9c0-5911-4aa0-8d80-66dfc35f36ce")
	)
	(pad "6" thru_hole oval
		(at -2.275 0.22)
		(size 0.85 1.85)
		(drill oval 0.35 1.35)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "34030271-8d72-4896-876c-0c8a93c170e2")
	)
	(pad "6" thru_hole oval
		(at 4.875 0.22)
		(size 0.85 1.85)
		(drill oval 0.35 1.35)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "83ba3d31-a300-4e0c-af39-a79ed7723551")
	)
	(embedded_fonts no)
	(model "${MY_ADDITIONS}/micro_usb_vetical.STEP"
		(offset
			(xyz 1.3 -1.75 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
